## SECTION 110.9 – MANDATORY REQUIREMENTS FOR LIGHTING CONTROLS

### (a) All lighting control devices and systems and

All light sources subject to the requirements of Section 110.9 shall meet the following requirements:

1. Shall be installed only if the lighting control or light source complies with all of the applicable requirements of Section 110.9.

2. Lighting controls may be individual devices or systems consisting of two or more components.

### (b) All Lighting Controls.

Lighting controls listed in Section 110.9(b) shall comply with the requirements 'listed below; and all components of the system considered together as installed shall meet all applicable requirements for the application for which they are installed as required in Sections 130.0 through 130.5, 140.6 through 140.8, Section 141.0, and 150.0(k)

1. Time-Switch Lighting Controls.

All controls that provide time-switch functionality, including all automatic and astronomical time-switch controls, shall have program backup capabilities that prevent the loss of the device’s schedule for at least 7 days, and the device’s date and time for at least 72 hours if power is interrupted. In addition:

A. Time-Switch Controls installed in nonresidential buildings shall

i. For each connected load, be capable of providing manual override to each connected load and of resuming normally scheduled operation after a manual override is initiated within 2 hours; and

ii. Provide an automatic holiday shutoff feature that turns off all connected loads for at least 24 hours and then resumes normally scheduled operation.

B. Astronomical Time-Switch Controls shall:

i. Have sunrise and sunset prediction accuracy within plus‐or‐minus 15 minutes and timekeeping accuracy within 5 minutes per year;

ii. Be capable of displaying date, current time, sunrise time, sunset time, and switching times for each step during programming;

iii. Be capable of automatically adjusting for daylight savings time; and

iv. Have the ability to independently offset the on and off for each channel by at least 90 minutes before and after sunrise or sunset.

C. Multi-Level Time-Switch Controls shall include at least 2 separately programmable steps per zone.

D. Time-Switch Controls installed outdoors shall have setback functions that allow the lighting on each controlled channel to be switched or dimmed to lower levels. The set back functions shall be capable of being programmed by the user for at least one specific time of day.

2. Daylighting Controls.

Controls that provide automatic daylighting functionality shall:

A. Automatically return to its most recent time delay settings within 60 minutes of the last received input when left in calibration mode;

B. Have a set point control that easily distinguishes settings to within 10 percent of full scale adjustment;

C. Provide a linear response within 5 percent accuracy over the range of illuminance measured by the light sensor; and

D. Be capable of being calibrated in a manner that the person initiating the calibration is remote from the sensor during calibration to avoid influencing calibration accuracy, for example by having a light sensor that is physically separated from where the calibration adjustments are made.

3. Dimmers. Controls that provide dimming functionality shall:

A. Be capable of reducing lighting power consumption by a minimum of 65% when at its lowest setting;

B. Provide reduced flicker operation, meaning that directly controlled light sources shall be provided electrical power such that the light output has an amplitude modulation of less than 30 percent for frequencies less than 200 Hz without causing premature lamp failure;

C. Provide an off setting that produces a zero lumen output; and

D. For wall box dimmers and associated switches designed for use in three way circuits, be capable of turning lights off, and on to the level set by the dimmer if the lights are off.

4. Occupant Sensing Controls. Occupant sensing controls include occupant sensors, motion sensors, and vacancy sensors, including those with a Partial-ON or Partial-OFF function. Occupant sensing controls shall:

A. Be capable of automatically turning the controlled lights in the area either off or down no more than 20 minutes after the area has been vacated;

B. For manual-on controls, have a grace period of no less than 15 seconds and no more than 30 seconds to turn on lighting automatically after the sensor has timed out; and

C. Provide a visible status signal that indicates that the device is operating properly, or that it has failed or malfunctioned. The visible status signal may have an override that turns off the signal.

EXCEPTION to Section 110.9(b)4: Occupant Sensing Control systems may consist of a combination of single or multilevel Occupant, Motion, or Vacancy Sensor Controls, provided that components installed to comply with manual-on requirements shall not be capable of conversion by occupants from manual-on to automatic-on functionality.

5. Part-Night 'Outdoor Lighting Controls, as defined in Section 100.1, shall meet all of the following requirements:

A. Have sunrise and sunset prediction accuracy within +/- 15 minutes, using both light sensing and time measurement; and

B. Have the ability to reduce or turn off outdoor luminaire power at night as required in Section 130.2(c) ; and

C. Shall be programmable to reduce or turn off outdoor luminaire power at any time as determined by the user. Time-based scheduling control is allowed to be relative to both sunset and sunrise, and to the midpoint between sunset and sunrise.

6. Sensors used to detect occupants. Sensors that are used by occupant sensing controls to detect occupants shall meet all of the following requirements:

A. Sensors shall not incorporate switches or mechanical devices that allow the sensor to be disabled without changing the settings of the control.

B. Sensors that utilize ultrasonic radiation for detection of occupants shall:

i. comply with 21 C.F.R. part 1002.12;

ii. not emit audible sound; and

iii. not emit ultrasound in excess of the decibel levels shown in Table 110.9-A measured no more than five feet from the source, on axis.

C. Sensors that utilize microwave radiation for detection of occupants shall:

i. comply with 47 C.F.R. parts 2 and 15; and

ii. not emit radiation in excess of 1 milliwatt per square centimeter measured at no more than 5 centimeters from the emission surface of the device.

7. Indicator Lights. Indicator lights integral to lighting controls shall consume no more than one watt of power per indicator light.

### (c) Track Lighting Integral Current Limiter.

An integral current limiter for line-voltage track lighting shall be recognized for compliance with Part 6 only if it meets all of the following requirements:

1. Shall have the identical volt-ampere (VA) rating of the current limiter, as installed and rated for compliance with Part 6 clearly marked as follows; and:

A. So that it is visible for the enforcement agency’s field inspection without opening coverplates, fixtures, or panels; and

B. Permanently marked on the circuit breaker; and

C. On a factory-printed label that is permanently affixed to a nonremovable base-plate inside the wiring compartment.

2. Shall have a conspicuous factory installed label permanently affixed to the inside of the wiring compartment warning against removing, tampering with, rewiring, or bypassing the device; and

3. Each electrical panel from which track lighting integral current limiters are energized shall have a factory printed label permanently affixed and prominently located, stating the following: "NOTICE: Current limiting devices installed in track lighting integral current limiters connected to this panel shall only be replaced with the same or lower amperage. Adding track or replacement of existing current limiters with higher continuous ampere rating will void the track lighting integral current limiter certification, and will require resubmittal of compliance documentation to the enforcement agency responsible for compliance with the California Title 24, Part 6 Building Energy Efficiency Standards.”

### (d) Track Lighting Supplementary Overcurrent Protection Panel.

A Track Lighting Supplementary Overcurrent Protection Panel shall be used only for line-voltage track lighting and shall be recognized for compliance with Part 6 only if it meets all of the following requirements:

1. Shall be 'listed as defined in Section 100.1; and

2. Shall have a permanently installed label that is prominently located stating the following: "NOTICE: This Panel for Track Lighting Energy Code Compliance Only. The overcurrent protection devices in this panel shall only be replaced with the same or lower amperage. No other overcurrent protective device shall be added to this panel. Adding to, or replacement of existing overcurrent protective device(s) with higher continuous ampere rating, will void the panel listing and require resubmittal of compliance documentation to the enforcement agency responsible for compliance with the California Title 24, Part 6 Building Energy Efficiency Standards.”

#### TABLE 110.9-A - ULTRASOUND MAXIMUM DECIBEL VALUES

Mid-frequency of Sound Pressure Third-Octave Band (in kHz) | Maximum db Level within Third-Octave Band (in dB reference 20 micropascals)
Less than 20 | 80
20 or more to less than 25 | 105
25 or more to less than 31.5 | 110
31.5 or more | 115

NOTE: Authority: Sections 25213, 25218, 25218.5, 25402 and 25402.1, Public Resources Code. Reference: Sections 25007, 25008, 25218.5, 25310, 25402, 25402.1, 25402.4, 25402.5, 25402.8, and 52943, Public Resources Code