## JA8.6 Data Reporting

The following test data shall be submitted to the California Energy Commission in the format specified in Table JA-8. The entity submitting the filing shall keep all test data and documentation required for compliance for at least two years from the date of certification and shall provide copies of this documentation to the Energy Commission within 10 days of written request received from the Energy Commission.

#### TABLE JA-8. DATA TO BE RECORDED AND SUBMITTED TO THE CALIFORNIA ENERGY COMMISSION

Required Information | Permissible Answers | Compliance Threshold
Manufacturer, Model number, Description |  |
Light Source Type | LED, OLED, Fluorescent, HID, Incandescent, Other |
Product type | Omnidirectional lamp, Directional lamp, Decorative lamp, LED light engine, inseparable SSL luminaire, T20 lamp other |
Lab accredited by NVLAP or accreditation body operating in accordance with ISO/IEC 17011? | Yes/No | Yes
Initial Efficacy | Value (lumens/Watt) | ≥ 45 lumens/Watt
Power Factor at Full Rated Power | 0 – 1 Fraction | ≥ 0.90
Start time | Value (seconds) | ≤ 0.5 sec
Correlated Color Temperature (CCT) | Number Kelvin | ≤4000 Kelvin.
Color Rendering Index (CRI) | 0-100 | ≥ 90 for all products other than T20 lamps, ≥ 82 for T20 lamps
Color Rendering R9 (red) | 0-100 or below 0 | ≥ 50 for all products other than T20 lamps
Ambient or elevated temperature test for rated life, lumen maintenance, and survival rate | Ambient or Elevated |
Lumen maintenance | Value (percent), N/A | ≥ 86.7% after final testing, or 93.1 if reporting interim data
Interim or Final reporting | Interim or Final |
Rated life | Value (hours) | ≥ 15,000 hours
survival rate | Value (percent) | ≥ 90%
Minimum dimming level | Value (percent) | ≤ 10%
Dimming control compatibility | Forward Phase cut control, reverse phase cut, powerline carrier, digital, 0-10 VDC, other. | At least one type must be listed
NEMA SSL 7A compatible? | Yes/No, NA | If compatible with forward phase cut dimmer control, “Yes”. If not, “NA”.
Flicker: |  |
See JA10 Table 10-1 for flicker data requirements and permissible answers |  | <30% for frequencies of 200 Hz or below, at 100% light output
Audible Noise |  |
100% light output: Audible Noise | Value (dBA) | ≤ 24 dBA
20% light output: Audible Noise | Value (dBA) | ≤ 24 dBA
Marking: |  |
Marked in accordance with JA8.5 | Yes/No | Yes