## 9.2 Covered Occupancies

§110.10(a)

The nonresidential solar-ready requirements apply to:

• Hotel/motel occupancies with 10 stories or fewer.

• High-rise multifamily buildings with 10 stories or fewer.

• All other nonresidential buildings with three stories or fewer.

• See Example 9-3.

Mixed Occupancy Buildings: The Energy Standards apply to mixed occupancy buildings. Buildings with nonresidential space on the ground floor and multi-family residential floors above are common examples.