# Appendix B Excerpts from the Appliance Efficiency Regulations

#### Table T-1
Normal Impedance Ranges for Liquid-Immersed Transformers

Single‐phase | Three‐phase
kVA | Impedance (%) | kVA | Impedance (%)
10 | 1.0–4.5 | 15 | 1.0–4.5
15 | 1.0–4.5 | 30 | 1.0–4.5
25 | 1.0–4.5 | 45 | 1.0–4.5
37.5 | 1.0–4.5 | 75 | 1.0–5.0
50 | 1.5–4.5 | 112.5 | 1.2–6.0
75 | 1.5–4.5 | 150 | 1.2–6.0
100 | 1.5–4.5 | 225 | 1.2–6.0
167 | 1.5–4.5 | 300 | 1.2–6.0
250 | 1.5–6.0 | 500 | 1.5–7.0
333 | 1.5–6.0 | 750 | 5.0–7.5
500 | 1.5–7.0 | 1000 | 5.0–7.5
667 | 5.0–7.5 | 1500 | 5.0–7.5
833 | 5.0–7.5 | 2000 | 5.0–7.5
|  | 2500 | 5.0–7.5

#### Table T-2
Normal Impedance Ranges for Dry-Type Transformers

Single‐phase | Three‐phase
kVA | Impedance (%) | kVA | Impedance (%)
15 | 1.5–6.0 | 15 | 1.5–6.0
25 | 1.5–6.0 | 30 | 1.5–6.0
37.5 | 1.5–6.0 | 45 | 1.5–6.0
50 | 1.5–6.0 | 75 | 1.5–6.0
75 | 2.0–7.0 | 112.5 | 1.5–6.0
100 | 2.0–7.0 | 150 | 1.5–6.0
167 | 2.5–8.0 | 225 | 3.0–7.0
250 | 3.5–8.0 | 300 | 3.0–7.0
333 | 3.5–8.0 | 500 | 4.5–8.0
500 | 3.5–8.0 | 750 | 5.0–8.0
667 | 5.0–8.0 | 1000 | 5.0–8.0
833 | 5.0–8.0 | 1500 | 5.0–8.0
|  | 2000 | 5.0–8.0
|  | 2500 | 5.0–8.0

#### Table A-1
Commercial Refrigerator, Refrigerator-Freezer,
and Freezer Test Methods

| Appliance | Test Method |
Automatic commercial ice makers | 10 C.F.R. sections 431.133 and 431.134
Refrigerated bottled or canned beverage vending machines | 10 C.F.R. sections 431.293 and 431.294
Refrigerated buffet and preparation tables | ANSI/ASTM F2143-01
Other commercial refrigerators, refrigrator-freezers and freezers, with doors | 10 C.F.R. sections 431.63 and 431.64
Other commercial refrigerators, refrigrator-freezers and freezers, without doors , | 10 C.F.R. sections 431.63 and 431.64
Walk-in coolers and walk-in freezers | 10 C.F.R. sections 431.303 and 431.304
|  |  |  |  |

#### Table A-2
Standards for Non-Commercial Refrigerators, Refrigerator-Freezers, and Freezers

Product Class | Maximum Energy Use (kWh/year)* Equation
1. Refrigerator-freezers and refrigerators other than all-refrigerators with manual defrost | 7.99AV + 225.0 0.28av+ 225.0
1A. All-refrigerators -- manual defrost | 6.79AV + 193.6 0.24av + 193.6
2. Refrigerator-freezers—partial automatic defrost | 7.99AV + 225.0 0.28av+ 225.0
3. Refrigerator-freezers—automatic defrost with top-mounted freezer without an automatic icemaker | 8.0 7 AV + 233.7 0.285av + 233.7
3-Bl. Built-in refrigerator-freezer---automatic defrost with top-mounted freezer without an automatic ice maker | 9.15AV + 264.9 0.323av + 264.9
3l. Refrigerator-freezer---automatic defrost with top-mounted freezer with an automatic ice maker without through-the-door ice service | 8.0 7 AV + 317.7 0.285av + 317.7
3l-Bl Built-in refrigerator-freezers--automatic defrost with top-mounted freezer with an automatic ice maker without through-the-door ice service | 9.1 5 AV + 348.9 0.323av + 348.9
3A. All refrigerators—automatic defrost | 7.07 AV + 2 01.6 0.25av + 201.6.0
3A-Bl. Built-in All refrigerators—automatic defrost | 8.02 AV + 22 8.5 0.283av + 228.5
4. Refrigerator-freezer--automatic defrost with side-mounted freezer without an automatic ice maker | 8.51 AV + 297.8 0.301av + 297.8
4-Bl. Built-in refrigerator-freezers automatic defrost with side-mounted freezer without an automatic ice maker | 10.22 AV + 357.4 0.361av + 357.4
4l. Refrigerator-freezer automatic defrost with side-mounted freezer with an automatic ice maker without through-the-door ice service | 8.51 AV + 381.8 0301 + 381.8
4l-Bl. Built-in refrigerator-freezers automatic defrost with side-mounted freezer with an automatic ice maker without through-the-door ice service | 10.22A V + 441.4 0.361 + 441.4
5. Refrigerator-freezer automatic defrost with bottom-mounted freezer without an automatic icemaker | 8.85AV + 317.0 0.312av + 317.0
5-Bl. Built-in refrigerator-freezers automatic defrost with bottom-mounted freezer without an automatic icemaker | 9.40AV + 336.9 0.332av + 336.9
5l. Refrigerator-freezer automatic defrost with bottom-mounted freezer without an automatic icemaker without through-the-door ice service. | 8.85AV + 401.0 0.312av + 401.0
5l-Bl. Built-in refrigerator-freezers automatic defrost with bottom-mounted freezer without an automatic icemaker without through-the-door ice service. | 9.40AV + 420.9 0.332av + 420.9
5A. Refrigerator-freezer automatic defrost with bottom-mounted freezer with through-the-door ice service. | 9.25 AV + 475.4 0.327av + 475.4
5A-Bl. Built-in refrigerator-freezersautomatic defrost with bottom-mounted freezer with through-the-door ice service. | 9.83AV + 499.9 0.347av + 499.9
6. Refrigerator-freezer automatic defrost with top-mounted freezer with through-the-door ice service. | 8.40AV + 385.4 0.297av + 385.4
7. Refrigerator-freezer automatic defrost with side-mounted freezer with through-the-door ice service. | 8.54 AV + 432.8 0.302av + 432.8
7-Bl. Built-in refrigerator-freezers automatic defrost with side-mounted freezer with through-the-door ice service. | 10.25 AV + 502.6 0.362av + 502.6
8. Upright freezers with manual defrost | 5.57 AV + 193.7 0.197av + 193.7
9. Upright freezers with automatic defrost without an automatic icemaker | 8.62 AV + 228.3 0.305av + 228.3
9l. Upright freezers with automatic defrost with an automatic icemaker | 8.62 AV + 312.3 0.348av + 312.3
9-Bl. Built-in upright freezers with automatic defrost without an automatic icemaker | 9.86AV + 260.9 0.348av + 260.9
9l-Bl. Built-in upright freezers with automatic defrost with an automatic icemaker | 9.86AV + 344.9 0.348av + 344.9
10. Chest freezers and all other freezers except compact freezers | 7.29 AV + 107.8 0.257av + 107.8
10A. Chest freezers with automatic defrost | 10.24 AV + 148.1 0.362av + 148.1
11. Compact refrigerator-freezers and refrigerators other than all-refrigerators with manual defrost | 9.03AV + 252.3 0.319av + 252.3
11A. Compact all refrigerators---manual defrost | 7.84 AV + 219.1 0.277av + 219.1
12. Compact refrigerator-freezers--partial automatic defrost | 5.91A V + 335.8 0.209 + 335.8
13. Compact refrigerator-freezers--automatic defrost with top-mounted freezer | 11.80AV + 339.2 0.417av + 339.2
13l. Compact refrigerator-freezers--automatic defrost with top-mounted freezer with an automatic icemaker | 11.80AV + 423.2 0.417av + 423.2.2
13A. Compact all refrigerators---automatic defrost | 9.17AV + 259.3 0.324av + 259.3
14. Compact refrigerator-freezers--automatic defrost with side-mounted freezer | 6.82AV + 456.9 0.241av + 456.9
14l. Compact refrigerator-freezers--automatic defrost with side-mounted freezer with an automatic icemaker | 6.82AV + 540.9 0.241av + 540.9
15. Compact refrigerator-freezers--automatic defrost with bottom-mounted freezer | 11.80AV + 339.2 0.417av + 339.2
15l. Compact refrigerator-freezers--automatic defrost with bottom-mounted freezer with an automatic icemaker | 11.80AV + 423.2 0.417av + 423.2
16. Compact upright freezers with manual defrost | 8.65 AV + 225.7 0.306av + 225.7
17. Compact upright freezers with automatic defrost | 10.17 AV + 351.9 0.359av + 351.9
18. Compact chest freezers | 9.25 AV + 136.8 0.327av + 136.8
*AV = Adjusted total Volume, Expressed in ft3, as determined in 10 C.F.R. sections 430.23(a) (Appendix A to subpart B of part 430) and 430.23(b) (Appendix B to subpart B of part 430) *av = Adjusted total volume, expressed in Liters.

#### Table B-1
Room Air Conditioner, Room Air-Conditioning Heat Pump,
Packaged Terminal Air Conditioner, and Packaged Terminal Heat Pump Test Methods

Appliance | Test Method
R oom air conditioners and room air‐conditioning heat pumps | 10 C.F.R. section 430.23(f) (Appendix F to Subpart B of part 430)
Pckaged terminal air conditioners and packaged terminal heat pumps | 10 C.F.R. sections 431.95 and 431.96

#### Table C-1
Central Air Conditioner Test Methods

Appliance | Test Method
‘Computer Room Air Conditioners
evaporatively‐cooled | ANSI/ASHRAE 127‐2001 10 C.F.R. sections 431.95 and 431.96
air‐cooled, glycol‐cooled, water‐cooled
Other electric‐powered unitary air‐conditioners and electric powered heat pumps
‘Air‐cooled air conditioners and ‘air‐source heat pumps
< 65,000 Btu/hr, single‐phase | 10 C.F.R. section 430.23(m) (Appendix M to Subpart B of part 430)
< 65,000 Btu/hr, three‐phase | 10 C.F.R. sections 431.95 and 431.96
≥ 65,000 and < 760,000 Btu/hr | 10 C.F.R. sections 431.95 and 431.96
‘evaporatively‐cooled air conditioners < 240,000 Btu/h | 10 C.F.R. sections 431.95 and 431.96
‘water‐cooled air conditioners and water‐source heat pumps<240,000 Btu/hr | 10 C.F.R. sections 431.95 and 431.96
ground ’water‐source heat pumps | ARI/ISO‐13256‐1:1998
ground‐source closed‐loop heat pumps | ARI/ISO‐13256‐1:1998
Variable Refrigerant Flow Multi‐split Systems | 10 C.F.R. sections 431.95 and 431.96
‘Single Package Vertical Air Conditioners and Single Package Vertical Heat Pumps | 10 C.F.R. sections 431.95 and 431.96
’Gas‐fired ‘air conditioners and gas‐fired heat pumps | ANSI Z21.40.4‐1996 as modified by CEC, Efficiency Calculation Method for Gas‐Fired Heat Pumps as a New Compliance Option (1996)

#### Table D-1
High-Speed Small-Diameter Ceiling Fan Blade and Tip Speed Criteria

’Airflow Direction | Thickness (t) of Edges of Blades | Tip ‘Speed Threshhold
Mn | Inch | m/s | Feet per Minute
Downward Only | 4.8 > t ≥3.2 | 3/16 > t ≥ 1/8 | 16.3 | 3200
Downward Only | t ≥ 4.8 | t ≥ 3/16 | 20.3 | 4000
Reversible | 4.8 > t ≥3.2 | 3/16 > t ≥ 1/8 | 12.2 | 2400
Reversible | t ≥ 4.8 | t ≥ 3/16 | 16.3 | 3200

#### Table E-1
Gas and Oil Space Heater Test Methods

Appliance | Test Method
Central furnaces
< 225,000 Btu/hr, single phase | 10 C.F.R. section 430.23(n) (Appendix N to Subpart B of part 430)
< 225,000 Btu/hr, three phase | 10 C.F.R. section 430.23(n) (Appendix N to Subpart B of part 430) or 10 C.F.R. sections 431.75 and 431.76 (at manufacturer’s option)
≥ 225,000 Btu/hr | 10 C.F.R. sections 431.75 and 431.76
‘Gas infrared heaters
patio heaters | ASTM F2644‐07
high‐intensity infrared heaters | ANSI Z83.19‐2001
low‐intensity infrared heaters | ANSI Z83.20‐2001
Gas Duct Furnaces | ANSI Z83.8‐2002*
Boilers
< 300,000 Btu/hr | 10 C.F.R. section 430.23(n) (Appendix N to Subpart B of part 430)
≥ 300,000 Btu/hr | 10 C.F.R. sections 431.85 and 431.86
Wall furnaces, floor furnaces, and room heaters | 10 C.F.R. section 430.23(o) (Appendix O to Subpart B of part 430)

#### Table F-1
Water Heater Non-Residential Application Exclusions

’Water Heater Type | Indicator on non-residential application
‘Gas-fired Storage | Rated Input > 105 kBtu/hour; rated storage volume > 120 gallons
Oil-fired Storage | Rated ‘Input > 140 kBtu/hour; rated storage volume > 120 gallons>
Electric Instantaneous | Rated ‘Input > rated storage volume > 2 gallons>

#### Table F-2
Standards for Water Heaters Regulated Under 10 C.F.R. Section 430.32(d)

Product Class | Rated Storage Volume and Input Rating (if applicable) | Draw Pattern | Minimum Uniform Energy Factor*
Gas-Fired Storage Water Heater | ≥ 20 gallons and ≤ 55 gallons | Very small | 0.3456 – (0.0020 x Vr)
Low | 0.5982 – (0.0019 x Vr)
Medium | 0.6483 – (0.0017 x Vr)
High | 0.6920 – (0.0013 x Vr)
> 55 gallons and ≤ 100 gallons | Very small | 0.6470 – (0.0006 x Vr)
Low | 0.7689 – (0.0005 x Vr)
Medium | 0.7897 – (0.0004 x Vr)
High | 0.8072 – (0.0003 x Vr)
Oil-Fired Storage Water Heater | ≤ 50 gallons | Very small | 0.2509 – (0.0012 x Vr)
Low | 0.5330 – (0.0016 x Vr)
Medium | 0.6078 – (0.0016 x Vr)
High | 0.6815 – (0.0014 x Vr)
Electric Storage Water Heater | ≥ 20 gallons and ≤ 55 gallons | Very small | 0.8808 – (0.0008 x Vr)
Low | 0.9254 – (0.0003 x Vr)
Medium | 0.9307 – (0.0002 x Vr)
High | 0.9349 – (0.0001 x Vr)
> 55 gallons and ≤ 120 gallons | Very small | 1.9236 – (0.0011 x Vr)
Low | 2.0440 – (0.0011 x Vr)
Medium | 2.1171 – (0.0011 x Vr)
High | 2.2418 – (0.0011 x Vr)
Tabletop Water Heater | ≥ 20 gallons and ≤ 120 gallons | Very small | 0.6323 – (0.0058 x Vr)
Low | 0.9188 – (0.0031 x Vr)
Medium | 0.9577 – (0.0023 x Vr)
High | 0.9884 – (0.0016 x Vr)
Instantaneous Gas-fired Storage Water Heater | < 2 gallons and > 50,000 Btuh | Very small | 0.80
Low | 0.81
Medium | 0.81
High | 0.81
Instantaneous Electric Water Heater | < 2 gallons | Very small | 0.91
Low | 0.91
Medium | 0.91
High | 0.92
Grid-Enabled Water Heater | > 75 gallons | Very small | 1.0136 – (0.0028 x Vr)
Low | 0.9984 – (0.0014 x Vr)
Medium | 0.9853 – (0.0010 x Vr)
High | 0.9720 – (0.0007 x Vr)
*Vr = Rated Storage Volume in gallons

#### Table G-1
Standards for Fossil Fuel-Fired Pool Heaters

Appliance | Effective Date | Minimum Thermal ‘Efficiency (%)
‘Gas-Fired ‘Pool Heaters | April 16, 2013 | 82
-Oil-Fired Pool Heaters | January 1, 1990 | 78

#### Table R-1
Cooking Product and Food Service Equipment Test Methods

Appliance | Test Method
Cooking products that are consumer products | 10 C.F.R. section 430.23(i) (Appendix I to Subpart B of part 430)
Combined cooking products | 10 C.F.R. section 430.23(i) (Appendix I to Subpart B of part 430)
Commercial hot food holding cabinets | ANSI/ASTM F2140-01 (Test for idle energy rate-dry test) and US EPA’s Energy Star Guidelines, “Measuring Interior Volume” (Test for interior volume)
Commercial convection ovens | ANSI/ASTM F1496-99 (Test for energy input rate and idle energy consumption only)
Commercial range tops | ANSI/ASTM F1521-96 (Test for cooking energy efficiency only)

#### Table A-3
Standards for Miscellaneous Refrigeration Products
Commercial Refrigerators, Commercial Refrigerator‐Freezers, and Commercial Freezers.

Product Class | Minimum Annual Energy Use (AEU) (kWh/Year)
Coolers
Built-in Compact Cooler | 7.88Av + 155.8
Built-in Cooler
Freestanding Compact Cooler
Freestanding Cooler
Combination Coolers
Combination Cooler with all refrigerator-automatic defrost | 4.57AV + 130.4
Built-in combination cooler with all refrigerator-automatic defrost | 5.19AV + 147.8
Combination Cooler with upright freezers with automatic defrost without an automatic ice maker | 5.58AV + 147.7
Built-in combination cooler with upright freezers with automatic defrost without an automatic ice maker | 6.38AV + 168.8
Combination Cooler with upright freezer with automatic defrost with an automatic ice maker | 5.58AV + 231.7
Built-in combination cooler with upright freezer with automatic defrost with an automatic ice maker | 6.38AV + 252.8
Compact combination cooler with all refrigerator-automatic defrost | 5.93AV + 193.7
Built-in compct combination cooler with all refrigerator-automatic defrost | 6.52AV + 213.1
AV= Adjusted total volume, expressed in ft3, as calculated according to 10 C. F. R. Appendix A to subpart B of part 430.

Table A-4
Standards for Commercial Refrigerators, Refrigerator-Freezers
with a Self-Contained Condensing Unit That are Not Commercial Hybrid Units

Equipment Category and Effective Date | Condensing Unit Configuration | Equipment Family | Rating Temperature (°F) | Operating Temperature (°F) | Equipment Class Designation* | Maximum Daily Energy Consumption (kWh)
Refrigerators and Freezers | Self Contained (SC) | Vertical Closed Transparent (VCT) | 38 (M) 0 (L) | ≥ 32 < 32 | VCT, SC, M VCT, SC, L | 0.1 × V + 0.86 0..29 × V + 2.95
Vertical Closed Solid (VCS) | 38 (M) 0 (L) | ≥ 32 < 32 | VCS, SC, M VCS, SC, L | 0.05 × V + 1.36 0.22 × V + 1.38
Horizontal Closed Transparent (HCT) | 38 (M) 0 (L) | ≥ 32 < 32 | HCT, SC, M HCT, SC, L | 0.06 × V + 0.37 0.08 × V + 1.23
Horizontal Closed Solid (HCS) | 38 (M) 0 (L) | ≥ 32 < 32 | HCS, SC, M HCS, SC, L | 0.05 × V + 0.91 0.06 × V + 1.12
Service Over Counter (SOC) | 38 (M) 0 (L) | ≥ 32 < 32 | SOC, SC, M SOC, SC, L | 0.51 x TDA + 1.0 1.10 × TDA + 2.10
Refrigerators with transparent doors | Self Contained (SC) | Pull Down PD) | 38 (P) | ≥ 32 | PD, SC, M | 0.11 × V + 0.81
Refrigerators and Freezers without Doors | Self Contained (SC) | Vertical Open (VOP) | 38 (M) 0 (L) | ≥ 32 < 32 | VOP, SC, M VOP, SC, L | 1.69 × TDA + 4.71 4.25 × TDA +11.82
Semivertical Open (SVO) | 38 (M) 0 (L) | ≥ 32 < 32 | SVO, SC, M SVO, SC, L | 1.70 × TDA + 4.59 4.26 × TDA +11.51
Horizontal Open (HZO) | 38 (M) 0 (L) | ≥ 32 < 32 | HZO, SC, M HZO, SC, L | 0.72 × TDA + 5.55 1.90 × TDA + 7.08
* The meaning of the letters in this column is indicated in the Condensing Unit Configuration, Equipment Family, and Rating Temperature (°F) columns to the left.

#### Table A-5
Standards for Commercial Refrigerators and Freezers
with a Remote Condensing Unit That are Not Commercial Hybrid Units

Equipment Category | Condensing Unit Configuration | Equipment Family | Rating Temperature (°F) | Operating Temperature (°F) | Equipment Class Designation* | Maximum Daily Energy Consumption (kWh)
Refrigerators and Freezers | ‘Remote (RC) | Vertical Open (VOP) | 38 (M) 0 (L) | ≥ 32 < 32 | VOP, RC, M VOP, RC, L | 0.64 × TDA + 4.07 2.2 0 × TDA + 6.85
Semivertical Open (SVO) | 38 (M) 0 (L) | ≥ 32 < 32 | SVO, RC, M SVO, RC, L | 0..66 × TDA + 3.18 2.2 0 × TDA + 6.85
Horizontal Open (HZO) | 38 (M) 0 (L) | ≥ 32 < 32 | HZO, RC, M HZO, RC, L | 0.35 × TDA + 2.88 0.5 5 × TDA + 6.88
Vertical Closed Transparent (VCT) | 38 (M) 0 (L) | ≥ 32 < 32 | VCT, RC, M VCT, RC, L | 0..15 × TDA + 1.95 0.49 × TDA + 2.61
Horizontal Closed Transparent (HCT) | 38 (M) 0 (L) | ≥ 32 < 32 | HCT, RC, M HCT, RC, L | 0.16 × TDA + 0.13 0.34 × TDA + 0.26
Vertical Closed Solid (VCS) | 38 (M) 0 (L) | ≥ 32 < 32 | VCS, RC, M VCS, RC, L | 0.1 0 × V + 0.26 0.2 1 × V + 0.54
Horizontal Closed Solid (HCS) | 38 (M) 0 (L) | ≥ 32 < 32 | HCS, RC, M HCS, RC, L | 0.1 0 × V + 0.26 0.2 1 × V + 0.54
Service Over Counter (SOC) | 38 (M) 0 (L) | ≥ 32 < 32 | SOC, RC, M SOC, RC, L | 0..44 × TDA + 0.11 0.93 × TDA + 0.22
* The meaning of the letters in this column is indicated in the Condensing Unit Configuration, Equipment Family, and Rating Temperature (°F) columns to the left.

#### Table A-7
Standards for Cube Type Automatic Commercial Ice Makers
Manufactured on or After January 1, 2010 and before January 28, 2018

Equipment type | Type of cooling | Harvest rate (lbs ice /24 hours) | Maximum ‘energy use (kWh/100 lbs ice) | Maximum condenser water use* (gal/100 lbs ice)
Ice Making Head | Water | < 500 | 7.80–0.0055H | 200–0.022H.
≥ 500 and < 1436 | 5.58–0.0011H | 200–0.022H.
≥ 1436 | 4.0 | 200–0.022H.
Ice Making Head | Air | < 450 | 10.26–0.0086H | Not applicable.
≥ 450 | 6.89-0.0011H | Not applicable.
Remote Condensing (but not remote compressor) | Air | < 1000 | 8.85–0.0038H | Not applicable.
≥ 1000 | 5.1 | Not applicable.
Remote Condensing and Remote Compressor) | < 934 | 8.85–0.0038H | Not applicable.
≥ 934 | 5.3 | Not applicable.
Self Contained | Water | < 200 | 11.40-0.019H | 191–0.0315H.
≥ 200 | 7.6 | 191–0.0315H.
Self Contained | Air | < 175 | 18.0–0.0469H | Not applicable.
≥ 175 | 9.8 | Not applicable.
H Harvest rate in pounds per 24 hours. *Water use is for the condenser only and does not include potable water used to make ice.

#### Table B-2
Standards for Room Air Conditioners and Room Air-Conditioning
Heat Pumps Manufactured on or after June 1, 2014

Appliance | Louvered Sides | Cooling Capacity (Btu/hr) | Minimum EER
Room ‘Air Conditioner | Yes | < 6,000 | 11.0
Room Air Conditioner | Yes | ≥ 6,000 – 7,999 | 11.0
Room Air Conditioner | Yes | ≥ 8,000 – 13,999 | 10.9
Room Air Conditioner | Yes | ≥ 14,000 – 19,999 | 10.7
Room Air Conditioner | Yes | ≥ 20,000 – 27,999 | 9.4
Room Air Conditioner | Yes | ≥ 28,000 | 9.0
Room Air Conditioner | No | < 6,000 | 10.0
Room Air Conditioner | No | ≥ 6,000 – 7,999 | 10.0
Room Air Conditioner | No | ≥ 8,000 – 1 0,999 | 9.6
Room Air Conditioner | No | ≥ 11,000 – 13,999 | 9.5
Room Air Conditioner | No | ≥ 14,000 – 19,999 | 9.3
Room Air Conditioner | No | ≥20,000 | 9.4
Room Air Conditioning Heat Pump | Yes | < 20,000 | 9.8
Room Air Conditioning Heat Pump | Yes | ≥20,000 | 9.3
Room Air Conditioning Heat Pump | No | < 14,000 | 9.3
Room Air Conditioning Heat Pump | No | ≥14,000 | 8.7
Casement‐Only Room Air Conditioner | Either | Any | 9.5
Casement‐Slider Room Air Conditioner | Either | Any | 10.4

#### Table B-3
Standards for Non-Standard Size Packaged Terminal Air Conditioners
and Non-Standard Size Packaged Terminal Heat Pumps Manufactured On or after October 7, 2010

Appliance | Cooling Capacity (Btu/hr) | Minimum ‘Efficiency
Minimum EER | Minimum COP
Packaged terminal air conditioners | < 7,000 | 9.4 | —
> 7,000 and < 15,000 | 10.9 – (0.213 x Cap1) | —
> 15,000 | 7.7 | —
Packaged terminal ‘heat pumps | < 7,000 | 9.3 | 2.7
> 7,000 and < 15,000 | 10.8 – (0.213 x Cap1) | 2.9 ‐ (0.0 26 x Cap1)
> 15,000 | 7.6 | 2.5
1Cap means cooling capacity in thousand British thermal units per hour (Btu/h) at 95°F outdoor dry-bulb

#### Table C-2
Air Filter Test Methods

Appliance | Test Method
Air Filter Pressure Drop | AHRI 680-2009 or ASHRAE 52.2-2012
Minimum ’Efficiency Reporting Value (MERV) | ASHRAE 52.2-2012
Air Filter Particle Size Efficiency | AHRI 680-2009 or ASHRAE 52.2-2012
Dust Holding Capacity | AHRI 680-2009 or ASHRAE 52.2-2012
*MERV not reportable for models being tested to AHRI 680-2009 only.

#### Table C-3
Standards for Single Phase Air-Cooled Air Conditioners with Cooling Capacity
Less than 65,000 Btu per Hour and Single Phase Air-Source Heat Pumps
with Cooling Capacity Less than 65,000 Btu per Hour, Not Subject to EPAct

Appliance | Minimum SEER | Minimum HSPF | Minimum EER | Average Off‐ Mode Power Consumption Pw. pff (watts)
Split system ‘air conditioners with rated cooling capacity < 45,000 Btu/hour¹ | 14.0 | — | 12.2 | 30
Split system air conditioners with rated cooling capacity ≥ 45,000 Btu/hour¹ | 14.0 | 11.7 | 30
Split system heat pumps with rated cooling capacity < 45,000 Btu/hour¹ | 14.0 | 8.2 |  | 33
Split system heat pumps with rated cooling capacity ≥ 45,000 Btu/hour¹ |  | 33
Single package air conditioners1 | 14.0 |  | 11.0 | 30
Single package heat pumps | 14.0 | 8.0 |  | 33
Space constrained air conditioners – split system | 12.0 |  | — | 30
Space constrained heat pumps – split system | 12.0 | 7.4 | — | 33
Space constrained air conditioners – single package | 12.0 |  | — | 30
Space constrained heat pumps – single package | 12.0 | 7.4 | — | 33
Small duct, high velocity ‘air conditioner systems | 12.0 |  | — | 30
Small duct, high velocity ‘heat pump systems | 12.0 | 7.2 | — | 30
1 See 10 C.F.R. section 430.32(c) for less stringent federal standards applicable to these units that are manufactured on or after JANUARY 1, 2015 and installed in states other than Arizona, California, Nevada, or New Mexico

#### Table C-4
Standards for Commercial Package Air-Conditioning and Heating Equipment
(Air-Cooled) Air Conditioners and Air-Source Heat Pumps Subject to EPAct
(Standards Effective January 1, 2010 do not apply to Single Package Vertical Air Conditioners)

Equipment Type | Cooling Capacity | Sub-category | Heating Type* | Efficiency Levels | Compliance date: Equipment Manufactured starting on
Small Commercial Package Air-Conditioning and Heating Equipment (Air-Cooled, 3-Phase, Split System) | < 65,000 Btu/h | AC | ALL | SEER = 13.0 | June 16, 2008
HP | SEER = 14.0 HSPF = 8.2 | January 1, 2017
Small Commercial Package Air-Conditioning and Heating Equipment (Air-Cooled, 3-Phase, Single Package) | ≥ 135,000 Btu/h and < 240,000 Btu/h | AC | ALL | SEER = 14.0 | January 1, 2017
HP | SEER = 14.0 HSPF = 8.0 | January 1, 2017
Small Commercial Package Air-Conditioning and Heating Equipment (Air-Cooled) | ≥ 65,000 Btu/h and < 135,000 Btu/h | AC | E-N | EER = 11.2 | January 1, 20101
IEER = 12.9 | January 1, 20182
IEER = 14.8 | January 1, 2023
A-O | EER = 11.0 | January 1, 20101
IEER = 12.7 | January 1, 20182
IEER = 14.6 | January 1, 2023
HP | E-N | EER = 11.0 COP = 3.3 | January 1, 20101
IEER = 12.2 COP = 3.3 | January 1, 20182
IEER = 14.1. COP = 3.4 | January 1, 2023
A-O | EER = 10.8 COP = 3.3 | January 1, 20101
IEER = 12.0 COP = 3.3 | January 1, 20182
IEER = 13.9. COP = 3.4 | January 1, 2023
Large Commercial Package Air-Conditioning and Heating Equipment (Air-Cooled) | ≥ 135,000 Btu/h and < 240,000 Btu/h | AC | E-N | EER = 11.0 | January 1, 20101
IEER = 12.4 | January 1, 20182
IEER = 14.2 | January 1, 2023
A-O | EER = 10.8 | January 1, 20101
IEER = 12.2 | January 1, 20182
IEER = 14.0 | January 1, 2023
HP | E-N | EER = 10.6 COP = 3.2 | January 1, 20101
IEER = 11.6 COP = 3.2 | January 1, 20182
IEER = 13.5. COP = 3.3 | January 1, 2023
A-O | EER = 10.4 COP = 3.2 | January 1, 20101
IEER = 11.4 COP = 3.3 | January 1, 20182
IEER = 13.3. COP = 3.4 | January 1, 2023
Very Large Commercial Package Air-Conditioning and Heating Equipment (Air-Cooled) | ≥ 240,000 Btu/h and < 760,000 Btu/h | AC | E-N | EER = 10.0 | January 1, 20101
IEER = 11.6 | January 1, 20182
IEER = 13.2 | January 1, 2023
A-O | EER = 9.8 | January 1, 20101
IEER = 11.4 | January 1, 20182
IEER = 13.0 | January 1, 2023
HP | E-N | EER = 9.5 COP = 3.2 | January 1, 20101
IEER = 10.6 COP = 3.23 | January 1, 20182
IEER = 12.5 | January 1, 2023
A-O | EER = 9.3 COP = 3.2 | January 1, 20101
IEER = 10.4 COP = 3.23 | January 1, 20182
IEER = 12.3 | January 1, 2023
1 And manufactured before January 1, 2018. 2And manufactured before January 1, 2023 3COP standard remains in effect on and after January 1, 2023 * E-N = Electric Resistance Heating or No Heating A-O = All Other Types of Heating

#### Table C-5
Standards for Commercial Package Air Conditioning and Heating Equipment (Water-Cooled)
Air Conditioners, Commercial Package Air Conditioning and Heating Equipment (Evaporatively Cooled
Air Conditioners, and Small Commercial Package Water-Source Heat Pumps

Equipment Type | Cooling Capacity | Sub-category | Heating Type* | Efficiency Levels | Compliance date: Equipment Manufactured starting on
Small Commercial Package Air-Conditioning and Heating Equipment (Water-Cooled) | < 65,000 Btu/h | AC | ALL | EER = 12.1 | October 29, 2003
N-E | EER = 12.1 | June 1, 2013
A-O | EER = 11.9
Large Commercial Package Air-Conditioning and Heating Equipment (Water-Cooled) | ≥ 135,000 Btu/h and < 240,000 Btu/h | AC | N-E | EER = 12.5 | June 1, 2014
A-O | EER = 12.3
Very Large Commercial Package Air-Conditioning and Heating Equipment (Water-Cooled) | ≥ 240,000 Btu/h and < 760,000 Btu/h | AC | N-E | EER = 12.4 | June 1, 2014
A-O | EER = 12.2
Small Commercial Package Air-Conditioning and Heating Equipment (Evaporatively-Cooled) | < 65,000 Btu/h | AC | ALL | EER = 12.1 | October 29, 2003
≥ 65,000 Btu/h and < 135,000 Btu/h | N-E | EER = 12.1 | June 1, 2013
A-O | EER = 11.9
Large Commercial Package Air-Conditioning and Heating Equipment (Evaporatively-Cooled) | ≥ 135,000 Btu/h and < 240,000 Btu/h | AC | N-E | EER = 12.0 | June 1, 2014
A-O | EER = 11.8
Very Large Commercial Package Air-Conditioning and Heating Equipment (Evaporatively-Cooled) | ≥ 240,000 Btu/h and < 760,000 Btu/h | AC | N-E | EER = 11.9 | June 1, 2014
A-O | EER = 11.7
Small Commercial Package Air-Conditioning and Heating Equipment (Water-Source: Water-to-Air, Water-Loop) | < 17,000 Btu/h | HP | ALL | IEER = 12.2 COP = 4.3 | October 9, 2015
≥ 17,000 Btu/h and < 135,000 Btu/h | IEER = 13.0 COP = 4.3
* N-E = No Heating or Electric Resistance Heating A-O = All Other Types of Heating

#### Table D-2
Low-Speed Small-Diameter Ceiling Fan Blade and Tip Speed Criteria

’Airflow Direction | Thickness (t) of Edges of Blades | Tip ‘Speed Threshhold
Mn | Inch | m/s | Feet per Minute
Reversible | 4.8 > t ≥3.2 | 3/16 > t ≥ 1/8 | 12.2 | 2400
Reversible | t ≥ 4.8 | t ≥ 3/16 | 16.3 | 3200

#### Table E-2
Standards for Gas Wall Furnaces, Floor Furnaces, and Room Heaters

Appliance | Design Type | Capacity (Btu per hour) | Minimum AFUE (%)
Effective On or After April 16, 2013
Wall furnace | Fan | ≤ 42,000 | 75
Wall furnace | Fan | > 42,000 | 76
Wall furnace | Gravity | 27,000 | 65
Wall furnace | Gravity | > 27,000 and ≤ 46,000 | 66
Wall furnace | Gravity | > 46,000 | 67
Floor furnace | All | ≤ 37,000 | 57
Floor furnace | All | > 37,000 | 58
Room heater | All | ≤ 20,000 | 61
Room heater | All | > 20,000 and < 27,000 | 66
Room heater | All | > 2 7,000 and < 46,000 | 67
Room heater | All | > 46,000 | 68

#### Table E-3
Standards for Gas- and Oil-Fired Central Boilers
< 300,000 Btu/hour Input and Electric Residential Boilers

Appliance | Minimum AFUE (%) | Maximum Power Consumption
Effective September 1, 2012 | Effective January 15, 2021
AFUE | Standby | Off Mode
Gas steam boilers with single phase electrical supply | 801 | 821 | 8 | 8
Gas hot ‘water boilers with single phase electrical supply | 821, 2 | 841, 2 | 9 | 9
Oil steam ‘boilers with single phase electrical supply | 82 | 85 | 11 | 11
Oil hot water boilers with single phase electrical supply | 842 | 862 | 11 | 11
Electric steam residential boilers | NONE | NONE | 8 | 8
Electric hot water residential boilers | NONE2 | NONE2 | 8 | 8
¹ No constant burning pilot light design standard effective September 1, 2012. ² Automatic means for adjusting temperature design standard effective September 1, 2012. (Boilers equipped with tankless domestic water heating coils do not need to comply with this requirement.)
|  |  |  |  |  |  |

Table E-5
Standards for Commercial Gas- and Oil-Fired Central Furnaces

Appliance | Rated Input (Btu/hr) | Minimum Thermal Efficiency
January 1, 1994 | January 1, 2023
Gas central furnaces | ≥ 225,000 | 80 | 81
Oil central furnaces | ≥ 225,000 | 81 | 82

#### Table F-2
Standards for Water Heaters Regulated Under 10 C.F.R. Section 430.32(d)

Product Class | Rated Storage Volume and Input Rating (if applicable) | Draw Pattern | Minimum Uniform Energy Factor*
Gas-Fired Storage Water Heater | ≥ 20 gallons and ≤ 55 gallons | Very small | 0.3456 – (0.0020 x Vr)
Low | 0.5982 – (0.0019 x Vr)
Medium | 0.6483 – (0.0017 x Vr)
High | 0.6920 – (0.0013 x Vr)
> 55 gallons and ≤ 100 gallons | Very small | 0.6470 – (0.0006 x Vr)
Low | 0.7689 – (0.0005 x Vr)
Medium | 0.7897 – (0.0004 x Vr)
High | 0.8072 – (0.0003 x Vr)
Oil-Fired Storage Water Heater | ≤ 50 gallons | Very small | 0.2509 – (0.0012 x Vr)
Low | 0.5330 – (0.0016 x Vr)
Medium | 0.6078 – (0.0016 x Vr)
High | 0.6815 – (0.0014 x Vr)
Electric Storage Water Heater | ≥ 20 gallons and ≤ 55 gallons | Very small | 0.8808 – (0.0008 x Vr)
Low | 0.9254 – (0.0003 x Vr)
Medium | 0.9307 – (0.0002 x Vr)
High | 0.9349 – (0.0001 x Vr)
> 55 gallons and ≤ 120 gallons | Very small | 1.9236 – (0.0011 x Vr)
Low | 2.0440 – (0.0011 x Vr)
Medium | 2.1171 – (0.0011 x Vr)
High | 2.2418 – (0.0011 x Vr)
Tabletop Water Heater | ≥ 20 gallons and ≤ 120 gallons | Very small | 0.6323 – (0.0058 x Vr)
Low | 0.9188 – (0.0031 x Vr)
Medium | 0.9577 – (0.0023 x Vr)
High | 0.9884 – (0.0016 x Vr)
Instantaneous Gas-fired Storage Water Heater | < 2 gallons and > 50,000 Btuh | Very small | 0.80
Low | 0.81
Medium | 0.81
High | 0.81
Instantaneous Electric Water Heater | < 2 gallons | Very small | 0.91
Low | 0.91
Medium | 0.91
High | 0.92
Grid-Enabled Water Heater | > 75 gallons | Very small | 1.0136 – (0.0028 x Vr)
Low | 0.9984 – (0.0014 x Vr)
Medium | 0.9853 – (0.0010 x Vr)
High | 0.9720 – (0.0007 x Vr)
*Vr = Rated Storage Volume in gallons

#### Table F-3
Standards for Water Heaters Regulated Under 42 U.S.C. section 6295(e)(1)

Product Class | Minimum Energy Factor*
Gas Water Heater1 | 0.62 – (0.0019 x Vr)
Oil Water Heater1 | 0.59 – (0.0019 x Vr)
Electric Water Heater1 | 0.95 – (0.00132 x Vr)
*Vr = Rated Storage Volume in gallons 1Applies to water heaters not covered under 10 C. F.R. section 430.32, including but not limited to storage water heaters >1 gal and < 20 gal (mini-tank water heaters) and booster water heaters. These standards will take effect on the effective date of a federal test procedure that converts Uniform Energy Factor (UEF) to Energy Factor for these products. If the Secretary adopts federal efficiency standards for water heaters regulated under 42 U. S. C. section 6295(e)(1), these standards shall not apply

#### Table H-1
Standards for Plumbing Fittings

Appliance | Maximum Flow Rate
Wash fountains | 2.2xrim space (inches)/20 gpm at 60psi
Metering ‘faucets | 0.25 gallons/cycle 1, 2
Metering faucets for wash fountains | 0.25 xrim space (inches)/20 gpm at 60 psi 1, 2
1Sprayheads with independently‐controlled orifices and metered controls. The maximum flow rate of each orifice that delivers a pre‐set volume of water before gradually shutting itself off shall not exceed the maximum flow rate for a metering faucet. 2Sprayheads with collectively‐controlled orifices and metered controls. The maximum flow rate of a sprayhead that delivers a pre‐set volume of water before gradually shutting itself off shall be the product of (a) the maximum flow rate for a metering ‘faucet and (b) the number of component lavatories (rim space of the lavatory in inches (millimeters) divided by 20 inches (508 millimeters)).

#### Table J-1
Percentage Time of Operation Table

Time Variable | Measurements Taken
P80,P50 | P80,NoP50 | NoP80,P50 | NoP80, NoP50
W100 | 0.2 | 0.35 | 0.45 | 1
W80 | 0.5 | 0.65 | 0 | 0
W50 | 0.3 | 0 | 0.55 | 0

#### Table J-2
Standards for Fluorescent Lamp Ballasts, Except for Certain Dimming Ballasts
Applicable to Models Described in Section 1605.1(j)(1) of this Article

BLE = A/(1 + b*average total lamp arc power ᴧ -C) Where A, B, and C are as follows:
Description | A | B | C
Instant start and rapid start ballasts (not classified as residential) that are designed to operate | 0.993 | 0.27 | 0.25
4‐foot medium bi‐pin lamps |  |  |
2‐foot U‐shaped lamps |  |  |
8-foot slimline lamps |  |  |
Programmed start ballasts (not classified as residential) that are designed to operate | 0.993 | 0.51 | 0.37
4‐foot medium bi‐pin lamps |  |  |
2‐foot U‐shaped lamps |  |  |
4‐foot minature bi‐pin standard output lamps |  |  |
4‐foot miniature bi‐pin high output lamps |  |  |
Instant start and rapid start ballasts (not classified as sign ballasts) that are designed to operate 8-foot high output lamps | 0.993 | 0.38 | 0.25
Programmed start ballasts (not classified as sign ballasts) that are designed to operate 8-foot high output lamps | 0.973 | 0.70 | 0.37
Sign ballasts that operate 8-foot high output lamps | 0.993 | 0.47 | 0.25
Instant start and rapid start residential ballasts that operate | 0.993 | 0.41 | 0.25
4‐foot medium bi‐pin lamps |  |  |
2‐foot U‐shaped lamps |  |  |
8-foot slimline lamps |  |  |
Programmed start residential ballasts that are designed to operate | 0.973 | 0.71 | 0.37
4‐foot medium bi‐pin lamps |  |  |
2‐foot U‐shaped lamps |  |  |

#### Table K-1
Optional Test Methods for State-Regulated LED Lamps and
LED State-Regulated Small Diameter Directional Lamps

Measurement | Test Procedure | Required or Optional
Flicker | Title 24, part 6, Joint Appendix 10 (2015), tested at both 100 percent and 20 percent output. Lamps with a percent amplitude modulation (percent flicker) less than 30 percent at frequencies less than 200Hz shall report “yes” for “reduced flicker operation” described in section 1606|tag=1606_a_Filing_of_Statements_ of this Article, otherwise report “no.” | Optional
Lumen Maintenance, Rated Life, and Survival Rate for Compliance with Title 24 Joint Appendix 8 and minimum dimming level | Title 24, part 6, Joint Appendix 8 (2015) | Optional
Audible Noise | ENERGY STAR Recommended Practice—Noise (2013) with the following modification: measurements shall be taken at 100 percent output as we as at 20 percent output if dimmable. | Optional

#### Table K-2
Standards for Federally-Regulated General Service Fluorescent Lamps
Manufactured On or After July 15, 2012

Appliance | Correlated Color Temperature | Minimum Average Lamp Efficacy (LPW)
Effective July 15, 2012 | Effective January 26, 2018
4‐foot medium bi‐pin lamps | ≤ 4,500K | 89 | 92.4
> 4,500K and ≤ 7,000K | 88 | 88.7
2‐foot U‐shaped lamps | ≤ 4,500K | 84 | 85.0
> 4,500K and ≤ 7,000K | 81 | 83.3
8-foot slimline lamps | ≤ 4,500K | 97 | 97.0
> 4,500K and ≤ 7,000K | 93 | 93.0
8‐foot high output lamps | ≤ 4,500K | 92 | 92.0
> 4,500K and ≤ 7,000K | 88 | 88.0
4-foot miniature bipin standard output | ≤ 4,500K | 86 | 95.0
> 4,500K and ≤ 7,000K | 81 | 89.3
4-foot miniature bipin high output | ≤ 4,500K | 76 | 82.7
> 4,500K and ≤ 7,000K | 72 | 76.9

#### Table K-3
Standards for Federally-Regulated Incandescent Reflector Lamps
Manufactured On or After July 15, 2012 and Sold Before January 1, 2020

‘Lamp Spectrum | Lamp Diameter (inches) | Rated Voltage | Minimum Average ‘Lamp Efficacy (LPW)1
Standard Spectrum | > 2.5 | ≥ 125 | 6.8 x P0.27
< 125 | 5.9 x P0.27
≤ 2.5 | ≥ 125 | 5.7 x P0.27
< 125 | 5.0 x P0.27
Modified Spectrum | > 2.5 | ≥ 125 | 5.8 x P0.27
< 125 | 5.0 x P0.27
≤ 2.5 | ≥ 125 | 4.9 x P0.27
< 125 | 4.2 x P0.27
1 P = Rated Lamp Wattage, in Watts

#### Table K-4
Standards for Medium Base Compact Fluorescent Lamps Manufactured On or After
January 1, 2006, and Sold Before January 1, 2020

Factor | Requirements
‘Labeled Wattage (Watts) and Configuration¹ | Measured Initial Lamp Efficacy: lumens/watt must be at least²
Bare Lamp: Labeled Wattage < 15 Labeled Wattage ≥ 15 | 45.0 60.0
Covered Lamp (no reflector) Labeled Wattage < 15 15 ≥ Labeled Wattage < 19 19 ≥ Labeled Wattage < 25 Labeled Wattage ≥ 25 | 40.0 48.0 50.0 55.0
Lumen Maintenance at 1,000‐hour s | ≥90%
Lumen Maintenance at 40% of Lifetime2 | 80%
Rapid ‘Cycle Stress Test | Each l amp must be cycled once for every two hours of lifetime2. At least 5 lamps must meet or exceed the minimum number of ‘cycles.
Lifetime2 | ≥ 6,000
¹ Use labeled wattage to determine the appropriate efficacy requirements in this table; do not use measured wattage for this purpose ² Lifetime refers to a lifetime of a compact fluorescent lamp as defined in Section 1602(k)|t ag=1602_k_Lamps of this Article

#### Table K-5
Standards for Federally-Regulated General Service Incandescent Lamps Manufactured
On or After the Effective Date Shown Below, and Sold Before January 1, 2020

Rated Lumen Ranges | Maximum Rate Wattage | Minimum Rate Lifetime | Effective Date
1490 ‐ 2600 | 72 | 1,000 hours | January 1, 2012
1050 – 1489 | 53 | 1,000 hours | January 1, 2013
750 – 1049 | 43 | 1,000 hours | January 1, 2014
310 – 749 | 29 | 1,000 hours | January 1, 2014

#### Table K-6
Standards for Federally-Regulated Modified Spectrum General Service Incandescent Lamps
Manufactured On or After the Effective Date Shown Below, and Sold Before January 1, 2020

Rated Lumen Ranges | Maximum Rate Wattage | Minimum Rate Lifetime | Effective Date
1118 ‐ 1950 | 72 | 1,000 hours | January 1, 2012
788 ‐ 1117 | 53 | 1,000 hours | January 1, 2013
563 ‐ 787 | 43 | 1,000 hours | January 1, 2014
232 ‐ 562 | 29 | 1,000 hours | January 1, 2014

#### Table K-7
Standards for Federally Regulated Candelabra Base Incandescent Lamps and Intermediate
Base Incandescent Lamps Manufactured On or After January 1, 2012, and Sold Before January 1, 2020

Lamp Base Type | Maximum Rated Wattage
Candelabra | 60
Intermediate | 40

#### Table M-1
Standards for Traffic Signals for Vehicle and Pedestrian Control

Appliance | Maximum Wattage (at 74°C) | Nominal Wattage (at 25°C)
Traffic Signal Module Type:
1 2‐inch; Red Ball | 17 | 11
8‐inch; Red Ball | 13 | 8
12‐inch; Red Arrow | 12 | 9
12‐inch; Green Ball | 15 | 15
8‐inch; Green Ball | 12 | 12
12‐inch; Green Arrow | 11 | 11
Pedestrian Module Type:
Combination Walking Man/Hand | 16 | 13
Walking Man | 12 | 9
Orange Hand | 16 | 13

Table O
Standards for Dishwashers

Appliance | Effective May 30, 2013
Maximum ‘Energy Use (kWh/year) | Maximum ‘Water Use (gallons/cycle)
Compact ‘dishwashers | 222 | 3.5
Standard dishwashers | 307 | 5.0

#### Table P-1
Standards for Residential Clothes Washers Manufactured
On or After January 1, 2007 and Manufactured Before March 7, 2015

Appliance | Minimum Integrated Modified ‘Energy Factor | Maximum Integrated Water Factor
March 7, 2015 | January 1, 2018 | March 7, 2015 | January 1, 2018
Top‐loading, C ompact | 0.86 | 1.15 | 14.4 | 12.0
Top‐loading, S tandard | 1.29 | 1.57 | 8.4 | 6.5
Front‐loading, Compact | 1.13 | 1.13 | 8.3 | 8.3
Front‐loading, Standard | 1.84 | 1.84 | 4.7 | 4.7
|  |  |  |  |  |  |  |

#### Table P-2
Standards for Commercial Clothes Washers

Appliance | Minimum Modified Energy Factor | Maximum Water Factor
Effective January 8, 2013 | Effective January 8, 2013
Top-loading clothes washers | 1.60 | 8.5
Front-loading clothes washers | 2.00 | 5.5
| Modified Energy Factor (MEF) ft3/kWh/cycle | Integrated Water Factor (IWF) gal./ft3cycle
Effective January 1, 2018 | Effective January 1, 2018
Top-loading clothes washers | 1.35 | 8.8
Front-loading clothes washers | 2.00 | 4.1

#### Table P-3 Standards for Commercial Clothes Washers

Appliance | Minimum Modified Energy Factor | Maximum Water Factor
Effective January 1, 2007 | Effective January 8, 2013 | Effective January 1, 2007 | Effective January 8, 2013
Top‐loading clothes washers | 1.26 | 1.60 | 9.5 | 8.5
Front‐loading clothes washers | 1.26 | 2.00 | 9.5 | 5.5

#### Table Q
Standards for Vented Electric Clothes Dryers, Ventless Electric Clothes Dryers, and
Vented Gas Clothes Dryers Manufactured On or After January 1, 2015

Appliance | Minimum Combined Energy Factor (lbs/kWh)
Vented | Ventless
Electric, standard clothes dryers | 3.73 | ---
Electric, compact, 120 volt clothes dryers | 3.61 | ---
Electric, compact, 240 volt clothes dryers | 3.27 | 2.55
Electric, combination washer-dryer | --- | 2.08
Gas clothes dryers | 3.30 | ---

#### Table S-1
Minimum Nominal Full-Load Efficiencies of NEMA Design A, NEMA Design B and
IEC Design N Motors (Excluding Fire Pump Electric Motors) at 60 Hz

Motor Horsepower/ Standard Kilowatt Equivalent | Nominal Full‐Load Efficiency
2 pole | 4 pole | 6 pole | 8 pole
Enclosed | Open | Enclosed | Open | Enclosed | Open | Enclosed | Open
1/0.75 | 77.0 | 77.0 | 85.5 | 85.5 | 82.5 | 82.5 | 75.5 | 75.5
1.5/1.1 | 84.0 | 84.0 | 86.5 | 86.5 | 87.5 | 86.5 | 78.5 | 77.0
2/1.5 | 85.5 | 85.5 | 86.5 | 86.5 | 88.5 | 87.5 | 84.0 | 86.5
3/2.2 | 86.5 | 85.5 | 89.5 | 89.5 | 89.5 | 88.5 | 85.5 | 87.5
5/3.7 | 88.5 | 86.5 | 89.5 | 89.5 | 89.5 | 89.5 | 86.5 | 88.5
7.5/5.5 | 89.5 | 88.5 | 91.7 | 91.0 | 91 | 90.2 | 86.5 | 89.5
10/7.5 | 90.2 | 89.5 | 91.7 | 91.7 | 91 | 91.7 | 89.5 | 90.2
15/11 | 91.0 | 90.2 | 92.4 | 93.0 | 91.7 | 91.7 | 89.5 | 90.2
20/15 | 91.0 | 91.0 | 93.0 | 93.0 | 91.7 | 92.4 | 90.2 | 91.0
25/18.5 | 91.7 | 91.7 | 93.6 | 93.6 | 93.0 | 93.0 | 90.2 | 91.0
30/22 | 91.7 | 91.7 | 93.6 | 94.1 | 93.0 | 93.6 | 91.7 | 91.7
40/30 | 92.4 | 92.4 | 94.1 | 94.1 | 94.1 | 94.1 | 91.7 | 91.7
50/37 | 93.0 | 93.0 | 94.5 | 94.5 | 94.1 | 94.1 | 92.4 | 92.4
60/45 | 93.6 | 93.6 | 95.0 | 95.0 | 94.5 | 94.5 | 92.4 | 93.0
75/55 | 93.6 | 93.6 | 95.4 | 95.0 | 94.5 | 94.5 | 93.6 | 94.1
100/75 | 94.1 | 93.6 | 95.4 | 95.4 | 95.0 | 95.0 | 93.6 | 94.1
125/90 | 95.0 | 94.1 | 95.4 | 95.4 | 95.0 | 95.0 | 94.1 | 94.1
150/110 | 95.0 | 94.1 | 95.8 | 95.8 | 95.8 | 95.4 | 94.1 | 94.1
200/150 | 95.4 | 95.0 | 96.2 | 95.8 | 95.8 | 95.4 | 94.5 | 94.1
250/186 | 95.8 | 95.0 | 96.2 | 95.8 | 95.8 | 95.8 | 95.0 | 95.0
300/224 | 95.8 | 95.4 | 96.2 | 95.8 | 95.8 | 95.8 |  |
350/261 | 95.8 | 95.4 | 96.2 | 95.8 | 95.8 | 95.8 |  |
400/298 | 95.8 | 95.8 | 96.2 | 95.8 |  |  |  |
450/336 | 95.8 | 96.2 | 96.2 | 96.2 |  |  |  |
500/373 | 95.8 | 96.2 | 96.2 | 96.2 |  |  |  |

#### Table T-3
Standards for Low-Voltage Dry-Type Distribution Transformers

Single phase | Three phase
kVA | ‘Efficiency (%)¹ | kVA | ‘Efficiency (%)¹
15 | 97.7 | 15 | 97.89
25 | 98.0 | 30 | 98.23
37.5 | 98.2 | 45 | 98.40
50 | 98.3 | 75 | 98.60
75 | 98.5 | 112.5 | 98.74
100 | 98.6 | 150 | 98.83
167 | 98.7 | 225 | 98.94
250 | 98.8 | 300 | 99.02
333 | 98.9 | 500 | 99.14
|  | 750 | 99.23
|  | 1000 | 99.28
¹ All e fficienc y values are at 35 percent of nameplate-rated load, determined according to the DOE Test Method for Measuring the Energy Consumption of distribution Transformers under of 10 C.F.R. part 431.
|  |  |  |  |

#### Table T-4
Standards for Liquid-Immersed Distribution Transformers

Single phase | Three phase
kVA | ‘Efficiency (%)¹ | kVA | ‘Efficiency (%)¹
10 | 98.70 | 15 | 98.65
15 | 98.82 | 30 | 98.83
25 | 98.95 | 45 | 98.92
37.5 | 99.05 | 75 | 99.03
50 | 99.11 | 112.5 | 99.11
75 | 99.19 | 150 | 99.16
100 | 99.25 | 225 | 99.23
167 | 99.33 | 300 | 99.27
250 | 99.39 | 500 | 99.35
333 | 99.43 | 750 | 99.40
500 | 99.49 | 1000 | 99.43
667 | 99.52 | 1500 | 99.48
833 | 99.55 | 2000 | 99.51
|  | 2500 | 99.53
¹ All e fficienc y values are at 50 percent of nameplate-rated load, determined according to the DOE Test Method for Measuring the Energy Consumption of distribution Transformers under Appenndix A to subpart K of 10 C.F.R. part 431.

#### Table T-5
Standards for Medium-Voltage Dry-Type Distribution Transformers
Manufactured On or After January 1, 2010 and Prior to January 1, 2016

Single phase | Three phase
BIL | BIL
kVA | 20‐45 kV efficiency¹ (%) | 46‐95 kV efficiency¹ (%) | ≥ 96 kV efficiency¹ (%) | kVA | 20‐45 kV efficiency¹ (%) | 46‐95 kV efficiency¹ (%) | ≥ 96 kV efficiency¹ (%)
15 | 98.10 | 97.86 |  | 15 | 97.50 | 97.18 |
25 | 98.33 | 98.12 |  | 30 | 97.90 | 97.63 |
37.5 | 98.49 | 98.30 |  | 45 | 98.10 | 97.86 |
50 | 98.60 | 98.42 |  | 75 | 98.33 | 98.1 3 |
75 | 98.73 | 98.57 | 98.53 | 112.5 | 98.52 | 98.3 6 |
100 | 98.82 | 98.67 | 98.63 | 150 | 98.6 5 | 98.51 |
167 | 98.96 | 98.83 | 98.80 | 225 | 98.82 | 98.69 | 98.5 7
250 | 99.07 | 98.95 | 98.91 | 300 | 98.93 | 98.81 | 98.6 9
333 | 99.14 | 99.03 | 98.99 | 500 | 99.09 | 98.99 | 98.8 9
500 | 99.22 | 99.12 | 99.09 | 750 | 99.21 | 99.12 | 9 9.02
667 | 99.27 | 99.18 | 99.15 | 1000 | 99.28 | 99.20 | 9 9.11
833 | 99.31 | 99.23 | 99.20 | 1500 | 99.37 | 99.30 | 99.21
|  |  |  | 2000 | 99.43 | 99.36 | 99.28
|  |  |  | 2500 | 99.47 | 99.41 | 99.33
¹ All e fficienc y values are at 50 percent of nameplate-rated load, determined according to the DOE Test Method for Measuring the Energy Consumption of distribution Transformers under Appendix A to subpart K of 10 C.F.R. part 431

#### Table U-1
Standards for Class A External Power Supplies That are Federally Regulated

Nameplate ‘Output | Minimum ‘Efficiency in Active Mode (Decimal equivalent of a Percentage)
Less than 1 watt | 0.5 * Nameplate Output
From 1 watt to not more than 51 watts | The sum of 0.09 times the Natural Logarithm of the Nameplate Output amd 0.5
Greater than 51 watts | 0.85
Not more than 250 watts | 0.5

#### Table A-9
Standards for Continuous Type Automatic Commercial Ice Makers
Manuf.actured on or After January 28, 2018

Equipment type | Type of cooling | Harvest rate (lbs ice/24 hours) | Maximum ‘energy use (kWh/100 lbs ice) | Maximum condenser water use* (gal/100 lbs ice)
Ice Making Head | Water | ≥50 and < 801 | 6.48-0.00267H | 180-0.0198H.
≥ 801 and < 2500 | 4.34 | 180-0.0198H.
≥ 2500 and< 4000 | 4.34 | 130.5
Air | ≥ 50 and < 310 | 9.19-0.00629H | Not applicable.
≥310 and < 820 | 8.23-0.0032H | Not applicable.
≥820 and < 4000 | 5.61 | Not applicable.
Remote Condensing (but not remote compressor) | Air | ≥ 50 and < 800 | 9.7-0.0058H | Not applicable.
≥ 800 and < 4000 | 5.06 | Not applicable.
Remote Condensing and Remote Compressor | ≥ 50 and < 800 | 9.9-0.0058H | Not applicable.
≥ 800 and < 4000 | 5.26 | Not applicable.
Self-Contained | Water | ≥ 50 and < 900 | 7.6-0.00302H | 153-0.0252H.
≥ 900 and < 2500 | 4.88 | 153-0.0252H.
≥ 2500 and < 4000 | 4.88 | 90
Air | ≥ 50 and < 200 | 14.22-0.03H | Not applicable.
≥ 200 and < 700 | 9.47-0.00624H | Not applicable.
≥ 700 and < 4000 | 5.1 | Not applicable.
H Harvest rate in pounds per 24 hours. *Water use is for the condenser only and does not include potable water used to make ice.

#### Table A-10
Standards for Walk-in Cooler and Walk-in Freezer Display Doors
Manufactured On or After June 5, 2017

Class Descriptor | Class | Maximum Daily Energy Consumption (kWh/day)*
Display Door, Medium Temperature | DD.M | 0.04 X Add + 0.41
Display Door, Low Temperature | DD.L | 0.15 X Add + 0.29
*Add represents the surface area of the display door.

#### Table A-12
Standards for Walk-in Cooler and Walk-in Freezer Refrigeration Systems
Manufactured On or After January 1, 2020

Class Descriptor | Class | Minimum AWEF (Btu/W-h
Dedicated Condensing, Medum Temperature, Indoor System | DC, M, I | 5.61
Dedicated Condensing, Medum Temperature, Outddor System | DC, M, 0 | 7.60

#### Table C-7
Standards for Computer Room Air Conditioners

Equipment type | Net sensible ‘cooling capacity (Btu/hr) | Minimum SCOP ‘efficiency | Compliance date:
Downflow unit | Upflow unit
Air‐Cooled | <65,000 | 2.20 | 2.09 | October 29, 2012
≥65,000 and <240,000 | 2.10 | 1.99 | October 29, 2013
≥240,000 and <760,000 | 1.90 | 1.79 | October 29, 2013
Water‐Cooled | <65,000 | 2.60 | 2.49 | October 29, 2012
≥65,000 and <240,000 | 2.50 | 2.39 | October 29, 2013
≥240,000 and <760,000 | 2.40 | 2.29 | October 29, 2013
Water‐Cooled with a Fluid Economizer | <65,000 | 2.55 | 2.44 | October 29, 2012
≥65,000 and <240,000 | 2.45 | 2.34 | October 29, 2013
≥240,000 and <760,000 | 2.35 | 2.24 | October 29, 2013
Glycol‐Cooled | <65,000 | 2.50 | 2.39 | October 29, 2012
≥65,000 and <240,000 | 2.15 | 2.04 | October 29, 2013
≥240,000 and <760,000 | 2.10 | 1.99 | October 29, 2013
Glycol‐Cooled with a Fluid Economizer | <65,000 | 2.45 | 2.34 | October 29, 2012
≥65,000 and <240,000 | 2.10 | 1.99 | October 29, 2013
≥240,000 and <760,000 | 2.05 | 1.94 | October 29, 2013

#### Table C-8
Standards for Variable Refrigerant Flow Multi-Split Air Conditioners and Heat Pumps

Equipment type | Cooling capacity | Heating type1 | ‘Efficiency level | Compliance date: Products manufactured on and after…
VRF Multi-Split ‘Air Conditioners (Air-Cooled) | <65,000 Btu/h | All | 13.0 SEER | June 16, 2008
≥65,000 Btu/h and <135,000 Btu/h | N-E | 11.2 EER | January 1, 2010
A-O | 11.0 EER | January 1, 2010
≥135,000 Btu/h and <240,000 Btu/h | N-E | 11.0 EER | January 1, 2010
AO | 10.8 EER | January 1, 2010
≥240,000 Btu/h and <760,000 Btu/h | N-E | 10.0 EER | January 1, 2010
A-O | 9.8 EER | January 1, 2010
VRF Multi-Split ‘Heat Pumps (Air-Cooled) | <65,000 Btu/h | All | 13.0 SEER 7.7 HSPF | June 16, 2008
≥65,000 Btu/h and <135,000 Btu/h | N-E | 11.0 EER 3.3 COP | January 1, 2010
A-O | 10.8 EER 3.3 COP | January 1, 2010
≥135,000 Btu/h and <240,000 Btu/h | N-E | 10.6 EER 3.2 COP | January 1, 2010
A-O | 10.4 EER 3.2 COP | January 1, 2010
≥240,000 Btu/h and <760,000 Btu/h | N-E | 9.5 EER 3.2 COP | January 1, 2010
A-O | 9.3 EER 3.3 COP | January 1, 2010
VRF Multi-Split Heat Pumps (Water Source) | <17,000 Btu/h | Without Heat Recovery | 12.0 EER 4.2 EER | October 29, 2012 October 29, 2003
With Heat Recovery | 11.8 EER 4.2 COP | October 29, 2012 October 29, 2003
≥17,000 Btu/h and <65,000 Btu/h | All | 12.0 EER 4.2 EER | October 29, 2003
≥65,000 Btu/h and <135,000 Btu/h | All | 12.0 EER 4.2 EER | October 29, 2003
≥135,000 Btu/h and <760,000 Btu/h | Without Heat Recovery | 10.0 EER 3.9 COP | October 29, 2013
With Heat Recovery | 9.8 EER 3.9 COP | October 29, 2013
1VRF Multi-Split Heat Pumps ( Air-Cooled ) with heat recovery fall under the category of “All Other Types of Heating” unless they also have electric resistance heating, in which case it falls under the category for “No Heating or Electric Resistance Heating.” *N-E = No Heating or Electric resistance heating A-O = All Other Types of Heating

#### Table E-7
Standards for Boilers

Appliance | Output (Btu/hr) | Standards
Minimum AFUE % | Minimum Combustion Efficiency % * | Maximum Standby Loss (watts)
Gas steam boilers with 3‐ phase electrical supply | < 300,000 | 75 | — | —
All other boilers with 3‐ phase electrical supply | < 300,000 | 80 | — | —
Natural gas, non‐packaged boilers | ≥300,000 | — | 80 | 147
LPG Non‐packaged boilers | ≥300,000 | — | 80 | 352
Oil, non‐packaged boilers | ≥ 300,000 | — | 83 | —
*At both maximum and minimum rated capacity, as provided and allowed by the controls.

#### Table E-8
Standards for Furnaces

Appliance | Application | Minimum Efficiency %
Central furnaces with 3‐phase electrical supply < 225,000 Btu/hour | Mobile Home | 75 AFUE
All others | 78 AFUE or 80 Thermal Efficiency (at manufacturer’s option)

#### Table E-9
Standards for Duct Furnaces

Appliance | Fuel | Standards
Minimum Thermal Efficiency %¹ | Maximum Energy Consumption during standby (watts)
At maximum rated capacity | At minimum rated capacity
Duct furnaces | Natural gas | 80 | 75 | 10
Duct furnaces | LPG² | 80 | 75 | 147
¹ As provided and allowed by the controls. 2 Designed expressly for use with LPG.

#### Table F-4
Standards for Water Heaters Regulated Under 10 C.F.R. Section 431.110(a)
(Excluding Residential-Duty Commercial Water Heaters)

Equipment Category | Size | Energy Conservation Standardsa
Maximum standby lossc (equipment manufactured on and after October 29, 2003)b | Minimum thermal efficiency (equipment manufactured on and after October 9, 2015)b (%)
Electric storage water heaters | All | 0.30 + 27/Vm (%/hr) | N/A
Gas-fired storage water heaters | ≤ 155,000 Btu/hr | Q/800 + 110(Vr) ½ (Btu/hr) | 80
> 155,000 Btu/hr | Q/800 + 110(Vr) ½ (Btu/hr) | 80
Oil-fired storage water heaters | ≤ 155,000 Btu/hr | Q/800 + 110(Vr) ½ (Btu/hr) | 80
> 155,000 Btu/hr | Q/800 + 110(Vr) ½ (Btu/hr) | 80
Gas-fired instantaneous water heaters and hot water supply boilers | < 10 gallons | N/A | 80
≥ 10 gallons | Q/800 + 110(Vr) ½ (Btu/hr) | 80
Oil-fired instantaneous water heaters and hot water supply boilers | < 10 gallons | N/A | 80
≥ 10 gallons | Q/800 + 110(Vr) ½ (Btu/hr) | 78
aVm is the measured storage volume (in gallons), and Vr is the rated volume (in gallons). Q is the nameplate input rate in Btu/hr. bFor hot water supply boilers with a capacity of less than 10 gallons: (1) the standards are mandatory for products manufactured on and after October 21, 2005; and (2) products manufactured prior to that date, and on or after October 23, 2003, must meet either the standards listed in Table F-3 or the applicable standards in Table E-4 of this Article for a “commercial packaged boiler.” cWater heaters and hot water supply boilers having more than 140 gallons of storage capacity need not meet the standby loss requirement if: (1) The tank surface area is thermally insulated to R-12.5 or more (2) a standing pilot light is not used; and (3) for gas or oil-fired storage water heaters, they have a fire damper or fan-assisted combustion.

#### Table H-2
Standards for Commercial Pre-rinse Spray Valves
Manufactured On or After January 28, 2019

Product Class (spray force in ounce force (ozf) | Maximum Flow Rate (gpm)
Product Class 1 ( ≤ 5.0 ozf) | 1.00
Product Class 2( > 5.0 ozf and ≤ 8.0 ozf) | 1.20
Product Class 3 ( > 8.0 ozf ) | 1.28

#### Table K-9
Standards for State-regulated LED Lamps

Effective Date | Minimum Compliance Score | Minimum Efficacy Lumens per Watt
January 1, 2018 | 282 | 68
July 1, 2019 | 297 | 80
The compliance score shall be calculated as the sum of the efficacy and 2.3 times the CRI of the lamp

#### Table K-10
Incandescent Wattage Equivalences
for State-regulated LED Lamps

Incandescent wattage equivalence | Minimum Lumen Output
40W | 310
60W | 750
75W | 1050
100W | 1490
150 | 2500

#### Table K-11 Standards for State-Regulated General Service Lamps -Tier II

Lumen Ranges | Minimum Lamp Efficacy | Minimum Rated Lifetime | Effective Date
All | 45 lumens per watt | 1,000 Hours | Jan, 1, 2018

#### Table K-12 Standards for State-Regulated Modified Spectrum General Service Incandescent Lamps -Tier I

Rated Lumen Ranges | Maximum Rated Wattage | Minimum Rated Lifetime | Effective Date
1118-1950 Lumens | 72 watts | 1,000 Hours | Jan 1, 2011
788-1117 Lumens | 53 watts | 1,000 Hours | Jan 1, 2012
563-787 Lumens | 43 watts | 1,000 Hours | Jan 1, 2013
232-562 Lumens | 29 watts | 1,000 Hours | Jan 1, 2013

Table L-1 Ultrasound Maximum Decibel Values

Mid-frequency of Sound Pressure Third-Octave Band (in kHz) | Maximum db Level within third-Octave Band(in dB reference 20 micropascals)
Less than 20 | 80
20 or more to less than 25 | 105
25 or more to less than 31.5 | 110
31.5 or more | 115

#### Table M-2
Standards for Traffic Signal Modules for Pedestrian Control
Sold or Offered for Sale in California

Type | At 25°C (77°F) | At 74°C (165.2°F)
Hand or ‘Don’t Walk’ sign or countdown. | 10 watts | 12 watts
Walking Person or ‘Walk’ sign | 9 watts | 12 watts

#### Table N-1
Standards for Metal Halide Lamp Fixtures Manufactured On or After February 10, 2017

Designed to be operated with ‘lamps of the following rated ‘lamp wattage | Tested input voltage‡‡ | Minimum standard equation‡‡%
≥ 50W and ≤ 100W | Tested at 480 V | (1/(1+1.24xP^(-0.351)))-0.020†;
≥ 50W and ≤ 100W | All others | 1/(1+1.24xP^(-0.351))
> 100W and < 150†;W | Tested at 480 V | (1/(1+1.24xP^(-0.351)))-0.020†;
> 100W and < 150†;W | All others | 1/(1+1.24xP^(-0.351))
> 500W and ≤ 1000W | Tested at 480 V | For >500W and ≤ 750W: 0.900
For >750W and ≤ 1000W: 0.000104xP+0.822
For >500W and ≤ 1000W: may not utilize a probe-start ballast
> 500W and ≤ 1000W | All others | For >500W and ≤ 750W: 0.910
For >750W and ≤ 1000W: 0.000104xP+0.832
For >500W and ≤ 1000W: may not utilize a probe-start ballast
† Includes 150 W fixtures specified in 10 C.F.R. section 431.326 paragraph (b)(3), that are fixtures rated only for 150 W lamps; rated for use in wet locations, as specified by the NFPA 70 section 410.4(A); and containing a ballast that is rated to operate at ambient air temperatures above 500 C, as specified by UL †† P is defined as the rated wattage of the lamp the fixture is designed to operate. ‡‡ Tested input voltage is specified in 10 C.F.R section 431.324.

#### Table N-2
Standards for Under-Cabinet Luminaires

Lamp Length (inches) | Minimum Ballast Efficacy Factor (BEF) for one lamp | Minimum Ballast Efficacy Factor (BEF) for two lamps
≤29 | 4.70 | 2.80
≥29 and ≤35 | 3.95 | 2.30
≥35 and ≤41 | 3.40 | 1.90
≥41 and ≤47 | 3.05 | 1.65
≥47 | 2.80 | 1.45

#### Table U-2
Standards for Direct Operation External Power Supplies

Powern Supply Type | Nameplate ‘Output Power Pout | Minimum Average ‘Efficiency in Active Mode* | Maximum Power in No-Load Mode [W]
Single-Voltage External AC-DC Power Supply, Basic Voltage | Pout ≤ 1 W | ≥ 0.5 x Pout + 0.16 | ≤ 0.100
1 W < Pout ≤ 49 W | ≥ 0.071 x In(Pout) - 0.0014 x Pout +0.67 | ≤ 0.100
49 W < Pout ≤ 250 W | ≥ 0.880 | ≤ 0.210
Pout >250 W | ≥ 0.875 | ≤ 0.500
Single-Voltage External AC-DC Power Supply, Low-Voltage | Pout ≤ 1 W | ≥ 0.517 x Pout + 0.87 | ≤ 0.100
1 W < Pout ≤ 49 W | ≥ 0.0834 x In(Pout) - 0.0014 x Pout +0.609 | ≤ 0.100
49 W < Pout ≤ 250 W | ≥ 0.870 | ≤ 0.210
Pout >250 W | ≥ 0.875 | ≤ 0.500
Single-Voltage External AC-AC Power Supply, Basic Voltage | Pout ≤ 1 W | ≥ 0.5 x Pout + 0.16 | ≤ 0.210
1 W < Pout ≤ 49 W | ≥ 0.071 x In(Pout) - 0.0014 x Pout +0.67 | ≤ 0.210
49 W < Pout ≤ 250 W | ≥ 0.880 | ≤ 0.210
Pout >250 W | ≥ 0.875 | ≤ 0.500
Single-Voltage External AC-AC Power Supply, Low-Voltage | Pout ≤ 1 W | ≥ 0.517 x Pout + 0.87 | ≤ 0.210
1 W < Pout ≤ 49 W | ≥ 0.834 x In(Pout) - 0.0014 x Pout +0.609 | ≤ 0.210
49 W < Pout ≤ 250 W | ≥ 0.880 | ≤ 0.210
Pout >250 W | ≥ 0.875 | ≤ 0.500
Multiple-Voltage External Power Supply | Pout ≤ 1 W | ≥ 0.497 x Pout + 0.067 | ≤ 0.300
1 W < Pout ≤ 49 W | ≥ 0.075 x In(Pout) +0.561 | ≤ 0.300
Pout > 49 W | ≥ 0.860 | ≤ 0.300
*Expressed as a decimal

T able U-3
Standards for All External Power Supplies Manufactured On or After February 10, 2016

Operation EPS Type | Class A EPS | Non-Class A EPS
Direct Operation EPS | Level VI: 10 C.F.R. 430.32 (w)(1)(ii) | Level VI: 10 C.F.R. 430.32 (w)(1)(i)
Indirect Operation EPS | Level VI: 10 C.F.R. 430.32 (w)(1)(i) | No standards

#### Table V-1
Interface Types and Scores for Expandability Score Calculation

Interface Type | Interface Score
USB 2.0 or less | 5
USB 3.0 or 3.1 Gen 1 | 10
USB 3.1 Gen 2 | 15
USB ports or Thunderbolt 3.0 or greater that can provide 100 or more watts of power | 100
USB ports or Thunderbolt 3.0 or greater that can provide from 60 or more to less than 100 watts of power | 60
USB ports or Thunderbolt 3.0 or greater that can provide from 30 or more to less than 60 watts of power | 30
Thunderbolt 3.0 or greater or USB ports that are not otherwise addressed in Table V-1 and that cannot provide 30 or more watts of power | 20
Unconnected USB 2.0 motherboard header | 10 per header
Unconnected USB 3.0 or 3.1 Gen 1 motherboard header | 20 per header
PCI slot other than PCIe x 16 (only count mechanical slots) | 25
PCIe x 16 (only count mechanical slots) | 75
Thunderbolt 2.0 or less | 20
M.2 (except key M) | 10
IDE, SATA, eSATA | 15
M.2, key M, SATA express, U.2 | 25
Integrated liquid cooling | 50
Either: 1) CPU and motherboard support for 4 or more channels of system memory and at least 8 GB of installed and compatible system memory; or 2) At least 8 GB of system memory installed on a 256 bit or greater memory interface. | 100

#### Table V-2
Standards for Consumer Audio and Video Equipment

Appliance Type | Effective Date | Maximum Power Usage (Watts)
Compact Audio Products | January 1, 2007 | 2 W in Audio standby‐passive mode for those without a permanently illuminated clock display 4 W in Audio standby‐passive mode for those with a permanently illuminated clock display
Digital Versatile Disc Players and Digital Versatile Disc Recorders | January 1, 2006 | 3 W in Video standby‐passive mode

#### Table W-1
Standards for Federally Regulated Battery Chargers
Manufactured on or after June 13, 2018

Product Class | Product Class Description | Rated Battery Energy (Ebatt**) | Special Characteristic or battery voltage | Maximym YEC (kWh/yr) (as a function of Ebatt**)
1 | Low-Energy | ≤ 5 Wh | Inductive Connection* | 3.04
2 | Low-Energy Low-Voltage | < 100 Wh | < 4 V | 0.1440 * Ebatt + 2.95
3 | Low-Energy Medium-Voltage | < 10 Wh | ≥ 4 V and ≤ 10V | 1.42 kWh/year
≥ 10 Wh | 0.0255 * Ebatt + 1.16
4 | Low-Energy High-Voltage |  | > 10 V | 0.11 * Ebatt + 3.18
5 | Medium-Energy Low-Voltage | ≥ 100 Wh and ≤ 3,000 Wh | < 20 V | 0.0257 * Ebatt + .0815
6 | Medium-Energy High-Voltage |  | ≥ 20 V | 0.0778 * Ebatt + 2.4
7 | High-Energy | >3,000 Wh |  | 0.0502 * Ebatt + 4.53
*Inductive connection and designed for use in a wet environment (e.g. electric toothbrushes). **Ebatt = Rated battery energy as determined in A part 429.39(a).

#### Table W-2
Standards for Large Battery Charger Systems

Performance Parameter | Standard
Charge Return Factor (CRF) | 100 percent, 80 percent Depth of discharge | CRF≤ 1.10
40 percent Depth of discharge | CRF ≤ 1.15
Power Conversion Efficiency | Greater than or equal to: 89 percent
Power Factor | Greater than or equal to: 0.90
Maintenance Mode Power (E b = battery capacity of tested battery) | Less than or equal to: 10 + 0.0012E b W
No Battery Mode Power | Less than or equal to: 10 W