###### Section 110.2(a) – Link to Tables 110.2-A-110.2-K

'Standards

Table 110.2-A AIR CONDITIONERS AND CONDENSING UNITS – MINIMUM EFFICIENCY REQUIREMENTS

Table 110.2-B HEAT PUMPS, MINIMUM EFFICIENCY REQUIREMENTS

Table 110.2-C AIR-COOLED GAS-ENGINE HEAT PUMPS

Table 110.2-D WATER CHILLING PACKAGES – MINIMUM EFFICIENCY REQUIREMENTS

Table 110.2-E PACKAGED TERMINAL AIR CONDITIONERS AND PACKAGED TERMINAL HEAT PUMPS – MINIMUM EFFICIENCY REQUIREMENTS

Table 110.2-F HEAT TRANSFER EQUIPMENT

Table 110.2-G PERFORMANCE REQUIREMENTS FOR HEAT REJECTION EQUIPMENT

Table 110.2-H ELECTRICALLY OPERATED VARIABLE REFRIGERANT FLOW (VRF) AIR CONDITIONERS MINIMUM EFFICIENCY REQUIREMENTS

Table 110.2-I Electrically Operated Variable Refrigerant Flow Air-to-Air and Applied Heat Pumps - Minimum Efficiency Requirements

Table 110.2-J Warm-Air Furnaces and Combination Warm-Air Furnaces/Air-Conditioning Units, Warm-Air Duct Furnaces, and Unit Heaters

Table 110.2-K Gas- and Oil-Fired Boilers, Minimum Efficiency requirements