## NA8.1 Luminaire Power

The following tables contain a limited list of lamp and ballast combinations. These tables provide an alternate voluntary option to the provision in Section 130.0(c) for determining luminaire power for any lamp and ballast combination specifically 'listed in Appendix NA8. This appendix is not intended to list all possible lamp and ballast combinations, and shall not to be used to determine luminaire power for any lighting system not specifically 'listed in this appendix.

#### Table NA8-1 – Fluorescent U-Tubes

Type | Lamps | Ballasts | System Watts
Number | Designation | Number | Designation | Description
2 ft. Fluorescent U-Tube T8 | 1 | FB31T8/F32T8U | 1 | ELECT NO | Electronic Normal Output | 39
2 | FB31T8/F32T8U | 1 | ELECT NO | Electronic Normal Output | 62
3 | FB31T8/F32T8U | 1 | ELECT NO | Electronic Normal Output | 92
1 | FB31T8/F32T8U | 1 | ELECT DIM | Electronic Dimming | 33
2 | FB31T8/F32T8U | 1 | ELECT DIM | Electronic Dimming | 64
3 | FB31T8/F32T8U | 1 | ELECT DIM | Electronic Dimming | 93
4 | FB31T8/F32T8U | 1 | ELECT DIM | Electronic Dimming | 116

NO = ballast factor 85 to 100%

#### Table NA8-2 – Fluorescent Linear Lamps T5

Type | Lamps | Ballasts | System Watts
Number | Designation | Number | Designation | Description
~23” Fluorescent Program Start T5 (14W) | 1 | F14T5 | 1 | ELECT | Elect. Program Start BF=1 | 18
2 | F14T5 | 1 | ELECT | Elect. Program Start BF=1 | 34
~34.5” Fluorescent Program Start T5 (21W) | 1 | F21T5 | 1 | ELECT | Elect. Program Start BF=1 | 27
2 | F21T5 | 1 | ELECT | Elect. Program Start BF=1 | 50
~46” Fluorescent Program Start T5 (28W) | 1 | F28T5 | 1 | ELECT | Elect. Program Start BF=1 | 30
2 | F28T5 | 1 | ELECT | Elect. Program Start BF=1 | 60
~58.5” Fluorescent Program Start T5 (35W) | 1 | F35T5 | 1 | ELECT | Elect. Program Start BF=1 | 40
2 | F35T5 | 1 | ELECT | Elect. Program Start BF=1 | 78
~23” Fluorescent Program Start T5 High Output (24W) | 1 | F24T5HO | 1 | ELECT | Elect. Program Start BF=1 | 29
2 | F24T5HO | 1 | ELECT | Elect. Program Start BF=1 | 55
~34.5” Fluorescent Program Start T5 High Output(39W) | 1 | F39T5 | 1 | ELECT | Elect. Program Start BF=1 | 43
2 | F39T5 | 1 | ELECT | Elect. Program Start BF=1 | 85
~46” Fluorescent Program Start T5 High Output (54W) | 1 | F54T5 | 1 | ELECT | Elect. Program Start BF=1 | 62
2 | F54T5 | 1 | ELECT | Elect. Program Start BF=1 | 121
1 | F54T5 | 1 | ELECT DIM | Elect. Dimming | 63
2 | F54T5 | 1 | ELECT DIM | Elect. Dimming | 125
~57.5” Fluorescent Program Start T5 High Output (80W) | 1 | ºF80T5 | 1 | ELECT | Elect. Program Start BF=1 | 90

#### Table NA8-3 – Fluorescent Rapid Start T-8

Type | Lamps | Ballasts | System Watts
Number | Designation | Number | Designation | Description
2 foot Fluorescent Rapid Start T8 (17W) Electronic Ballasts | 1 | F17T8 | 1 | ELECT NO | Electronic Normal Output | 22
2 | F17T8 | 1 | ELECT NO | Electronic Normal Output | 33
3 | F17T8 | 1 | ELECT NO | Electronic Normal Output | 53
3 | F17T8 | 2 | ELECT NO | Electronic Normal Output | 55
4 | F17T8 | 1 | ELECT NO | Electronic Normal Output | 63
2 foot Fluorescent Rapid Start T8 (17W) | 1 | F17T8 | 1 | ELECT DIM | Electronic Dimming | 20
2 | F17T8 | 1 | ELECT DIM | Electronic Dimming | 37
3 | F17T8 | 1 | ELECT DIM | Electronic Dimming | 56
4 | F17T8 | 1 | ELECT DIM | Electronic Dimming | 69
3 foot Fluorescent Rapid Start T8 (25W) Electronic Ballasts | 1 | F25T8 | 1 | ELECT NO | Electronic Normal Output | 27
2 | F25T8 | 1 | ELECT NO | Electronic Normal Output | 48
3 | F25T8 | 1 | ELECT NO | Electronic Normal Output | 68
4 | F25T8 | 1 | ELECT NO | Electronic Normal Output | 89
1 | F25T8 | 1 | ELECT RO | Electronic Reduced Output | 24
2 | F25T8 | 1 | ELECT RO | Electronic Reduced Output | 41
3 | F25T8 | 1 | ELECT RO | Electronic Reduced Output | 59
4 | F25T8 | 1 | ELECT RO | Electronic Reduced Output | 76
1 | F25T8 | 1 | ELECT HO | Electronic High Output | 29
2 | F25T8 | 1 | ELECT HO | Electronic High Output | 51
3 | F25T8 | 1 | ELECT HO | Electronic High Output | 74
1 | F25T8 | 1 | ELECT DIM | Electronic Dimming | 25
2 | F25T8 | 1 | ELECT DIM | Electronic Dimming | 49
3 | F25T8 | 1 | ELECT DIM | Electronic Dimming | 76
4 | F25T8 | 1 | ELECT DIM | Electronic Dimming | 96
4 foot Fluorescent Instant Start T8 (“Energy Saving” 30W) | 1 | F32T8/30ES | 1 | ELECT NO | Electronic Normal Output | 29
2 | F32T8/30ES | 1 | ELECT NO | Electronic Normal Output | 54
3 | F32T8/30ES | 1 | ELECT NO | Electronic Normal Output | 79
4 | F32T8/30ES | 1 | ELECT NO | Electronic Normal Output | 104
1 | F32T8/30ES | 1 | ELECT RO | Electronic Reduced Output | 27
2 | F32T8/30ES | 1 | ELECT RO | Electronic Reduced Output | 48
3 | F32T8/30ES | 1 | ELECT RO | Electronic Reduced Output | 70
4 | F32T8/30ES | 1 | ELECT RO | Electronic Reduced Output | 91
1 | F32T8/30ES | 1 | ELECT NO EE | EE Normal Output | 33
2 | F32T8/30ES | 1 | ELECT NO EE | Energy efficiency Normal Output | 52
3 | F32T8/30ES | 1 | ELECT NO EE | Energy efficiency Normal Output | 77
4 | F32T8/30ES | 1 | ELECT NO EE | Energy efficiency Normal Output | 101
1 | F32T8/30ES | 1 | ELECT RO EE | EE Reduced Output | 28
2 | F32T8/30ES | 1 | ELECT RO EE | EE Reduced Output | 45
3 | F32T8/30ES | 1 | ELECT RO EE | EE Reduced Output | 66
4 | F32T8/30ES | 1 | ELECT RO EE | EE Reduced Output | 88
4 foot Fluorescent Rapid Start T8 (32W) | 1 | F32T8 | 1 | ELECT NO | Electronic Normal Output | 32
2 | F32T8 | 1 | ELECT NO | Electronic Normal Output | 62
3 | F32T8 | 1 | ELECT NO | Electronic Normal Output | 93
4 | F32T8 | 1 | ELECT NO | Electronic Normal Output | 114
1 | F32T8 | 1 | EE NO | EE Normal Output | 35
2 | F32T8 | 1 | EE NO | EE Normal Output | 55
3 | F32T8 | 1 | EE NO | EE Normal Output | 82
4 | F32T8 | 1 | EE NO | EE Normal Output | 107
1 | F32T8 | 1 | ELECT RO | Electronic Reduced Output | 29
2 | F32T8 | 1 | ELECT RO | Electronic Reduced Output | 51
3 | F32T8 | 1 | ELECT RO | Electronic Reduced Output | 76
4 | F32T8 | 1 | ELECT RO | Electronic Reduced Output | 98
2 | F32T8 | 1 | ELECT HO | Electronic High Output | 77
3 | F32T8 | 1 | ELECT HO | Electronic High Output | 112
1 | F32T8 | 1 | EE RO | EE Reduced Output | 30
2 | F32T8 | 1 | EE RO | EE Reduced Output | 48
3 | F32T8 | 1 | EE RO | EE Reduced Output | 73
4 | F32T8 | 1 | EE RO | EE Reduced Output | 96
2 | F32T8 | 1 | ELECT TL | Electronic Two Level (50 & 100%) | 65
1 | F32T8 | 1 | ELECT DIM1 | Electronic Dimming | 35
2 | F32T8 | 1 | ELECT DIM1 | Electronic Dimming | 68
3 | F32T8 | 1 | ELECT DIM1 | Electronic Dimming | 102
1 | F32T8 | 1 | ELECT DIM2 | Electronic Dimming | 33
2 | F32T8 | 1 | ELECT DIM2 | Electronic Dimming | 64
3 | F32T8 | 1 | ELECT DIM2 | Electronic Dimming | 93
4 | F32T8 | 1 | ELECT DIM2 | Electronic Dimming | 116
5 foot Fluorescent Rapid Start T8 (40W) | 1 | F40T8 | 1 | ELECT | Electronic | 46
2 | F40T8 | 1 | ELECT | Electronic | 79
3 | F40T8 | 1 | ELECT | Electronic | 112

RO = ballast factor 70 to 85% NO = ballast factor 85 to 100% HO = ballast factor >100%

#### Table NA8-4 – Fluorescent Rapid Start High Output (HO) T8, 8 ft

Type | Lamps | Ballasts | System Watts
Number | Designation | Number | Designation | Description
8 foot Fluorescent Rapid Start T8 High Output (86W) | 1 | F96T8/HO | 1 | ELECT | Electronic | 88
2 | F96T8/HO | 1 | ELECT | Electronic | 160

HO = ballast factor >100%

#### Table NA8-5 – High Intensity Discharge

Type | Lamps | Ballasts | System Watts
Number | Designation | Number | Designation | Description
Metal Halide | 1 | M35/39 | 1 | MAG STD | Mag. Stand. | 58
1 | M35/39 | 1 | ELECT | Electronic | 44
1 | M50 | 1 | MAG STD | Mag. Stand. | 67
1 | M50 | 1 | ELECT | Electronic | 58
1 | M70 | 1 | MAG STD | Mag. Stand. | 95
1 | M70 | 1 | ELECT | Electronic | 86
1 | M100 | 1 | MAG STD | Mag. Stand. | 130
1 | M100 | 1 | ELECT | Electronic | 110
1 | M150 | 1 | MAG STD | Mag. Stand. | 185
1 | M150 | 1 | ELECT | Electronic | 168
1 | M175 | 1 | MAG STD | Mag. Stand. | 208
1 | M175 | 1 | ELECT | Electronic | 194
1 | M200 | 1 | MAG STD | Mag. Stand. | 232
1 | M250 | 1 | MAG STD | Mag. Stand. | 295
1 | M250 | 1 | ELECT | Electronic | 269
1 | M320 | 1 | MAG STD | Mag. Stand. | 368
1 | M320 | 1 | ELECT | Electronic | 343
1 | M360 | 1 | MAG STD | Mag. Stand. | 422
1 | M400 | 1 | MAG STD | Mag. Stand. | 452
1 | M400 | 1 | ELECT | Electronic | 430
1 | M450 | 1 | MAG STD | Mag. Stand. | 508
1 | M750 | 1 | MAG STD | Mag. Stand. | 818
1 | M1000 | 1 | MAG STD | Mag. Stand. | 1080
1 | M1500 | 1 | MAG STD | Mag. Stand. | 1605
High Pressure Sodium | 1 | S35 | 1 | MAG STD | Mag. Stand. | 47
1 | S50 | 1 | MAG STD | Mag. Stand. | 66
1 | S70 | 1 | MAG STD | Mag. Stand. | 91
1 | S100 | 1 | MAG STD | Mag. Stand. | 128
1 | S150 | 1 | MAG STD | Mag. Stand. | 188
1 | S200 | 1 | MAG STD | Mag. Stand. | 230
1 | S250 | 1 | MAG STD | Mag. Stand. | 295
1 | S400 | 1 | MAG STD | Mag. Stand. | 464
1 | S1000 | 1 | MAG STD | Mag. Stand. | 1100

#### Table NA8-6 –12 Volt Tungsten Halogen Lamps Including MR16,
Bi-pin, AR70, AR111, PAR36(Shall NOT apply to track lighting systems)

Type | Lamps | Ballasts | System Watts
Number | Designation | Number | Designation | Description
| 1 | 20 watt lamp | 1 | ELECT | Electronic Power Supply | 23
1 | 25 watt lamp | 1 | ELECT | Electronic Power Supply | 28
1 | 35 watt lamp | 1 | ELECT | Electronic Power Supply | 38
1 | 37 watt lamp | 1 | ELECT | Electronic Power Supply | 41
1 | 42 watt lamp | 1 | ELECT | Electronic Power Supply | 45
1 | 50 watt lamp | 1 | ELECT | Electronic Power Supply | 54
1 | 65 watt lamp | 1 | ELECT | Electronic Power Supply | 69
1 | 71 watt lamp | 1 | ELECT | Electronic Power Supply | 75
1 | 75 watt lamp | 1 | ELECT | Electronic Power Supply | 80
1 | 20 watt lamp | 1 | MAG | Mag. Transformer | 24
1 | 25 watt lamp | 1 | MAG | Mag. Transformer | 29
1 | 35 watt lamp | 1 | MAG | Mag. Transformer | 39
1 | 37 watt lamp | 1 | MAG | Mag. Transformer | 42
1 | 42 watt lamp | 1 | MAG | Mag. Transformer | 46
1 | 50 watt lamp | 1 | MAG | Mag. Transformer | 55
1 | 65 watt lamp | 1 | MAG | Mag. Transformer | 70
1 | 71 watt lamp | 1 | MAG | Mag. Transformer | 76
1 | 75 watt lamp | 1 | MAG | Mag. Transformer | 81