## JA2.2 California Design Location Data

The data contained in the following table was obtained through a joint effort by the Southern California Chapter and the Golden Gate Chapter of ASHRAE. It is reprinted here with the written permission of Southern California Chapter ASHRAE, Inc. The values for 1.0 percent drybulb and 1.0 percent mean coincident wetbulb (MCWB) are interpolated.

The data in Table 2-3 is developed from A full listing of design location data for California is contained in the ASHRAE publication SPCDX, Climate Data for Region X, Arizona, California, Hawaii, and Nevada (ISBN 200021, May 1982) and Supplement to Climatic Data for Region X, Arizona, California, Hawaii, Nevada (ISBN 20002956, November 1994). The publication may be ordered from:

Order Desk
Building News
10801 National Blvd.
Los Angeles, CA 90064
(888) 264-7483 or (310) 474-7771
http://www.bnibooks.com

Note to User: Table 2-3 is a large table. The links below open very slowly…please be patient.

Link to Table 2-3 – Design Day Data for California Cities

*Heating Degree Day is a unit, based on temperature difference and time, used in estimating fuel consumption and specifying nominal annual heating load of a building. For any one day when the mean temperature is less than 65ºF (18ºC), there exist as many degree days as there are Fahrenheit degrees difference in temperature between mean temperature for the day and 65ºF (18ºC).

KEY TO ABBREVIATIONS:

AFB Air Force Base

AFS Air Force Station

AP Airport

CO City/County Office

FD Fire Department

FS Fire Station

MCB Marine Corps Base

MCWB Mean Coincident Wet Bulb

NAS Naval Air Station

NM National Monument

PH Power House

RS Ranger Station